**Annex 4**

**Technical Compliance Table**

|  |  |
| --- | --- |
| **Minimum Description/Specification of goods** | **Compliance****Yes/No***(provide details)* |
| **Type**  | **Multi-Purpose Vehicle (MPV)** **9 seats, including driver**  |  |
| **Body** | Standard non-metallic white colour |  |
| Metallic structure divided virtually into three compartments (cab, passenger compartment and load compartment)  |  |
| Fully glazed  |  |
| **Year of manufacture**  | 2017-2018, brand new vehicle  |  |
| **Steering**  | * Left-hand drive;
* Hydraulic power assisted steering;
* Adjustable steering wheel
 |  |
| **Engine** |  |  |
| *Displacement*  | 1800-2000 cm3 |  |
| *Power*  | At least 140 HP at 3500-4500 rpm |  |
| *Torque*  | At least 350 Nm at 1500-2500 rpm |  |
| *Type*  | At least 4 cylinders |  |
| *Emission standard*  | EURO 5 or better  |  |
| *Fuel type* | Diesel  |  |
| *Consumption (combined cycle)* | Up to 8 l/100 km |  |
|  | Fuel filter with water separator |  |
| **Tank capacity**  | At least 70 l |  |
| **Transmission** | 6-speed manual transmission |  |
| Front-Wheel Drive (FWD) |  |
| **Doors and windows** | * 2 (two) doors in front (one for the driver, one for the passenger) with tinted windows;
* 1 (one) right side sliding door;
* 1 (one) rear door with dark tinted windscreen.
 |  |
|  | Fixed dark tinted windows in row 2 and row 3 (min 60% opacity) |  |
| **Seating** |  |  |
| *Type of seats\**  | * 1 (one) seat for driver with angle-adjustable armrests, adjustable head restraints and adjustable seat;
* 1 (one) double seats bench in front (for passenger(s)) with adjustable head restraints;
* 3-seater bench (1/3 2/3) in row 2, full size seats, removable;
* 3-seater bench in row 3, full size seats, removable.

**\* A different configuration of seats might be acceptable, provided that the last row of seats is removable** |  |
| *Upholstery*  | High resistant dark fabric/cloth  |  |
| **Interior equipment** | Automatic dual zone air conditioning/ climate control  |  |
| Non-slip floor covering  |  |
| **Dimensions** |  |  |
| *Wheelbase*  | At least 3200 mm (long wheelbase) |  |
| *Overall length*  | Up to 5400 mm |  |
| *Overall width*  | Up to 2500 mm |  |
| *Overall height*  | Up to 2000 mm |  |
| *Gross vehicle weight*  | Up to 3500 kg |  |
| *Payload*  | At least 1000 kg  |  |
| *Turning circle* | Up to 13 m |  |
| **Electronics** | Remote central locking |  |
| Front electric windows  |  |
| Electrically adjustable and heated door mirrors |  |
| Front and rear fog lamps  |  |
| Parking aid system (front and rear) |  |
| Metric instrument cluster (including at least speedometer, odometer, fuel gauge, seat belt warning light, clock, outside temperature display) |  |
| 3 x 12V sockets |  |
| Audio device with AM/FM radio tuner, USB interface, speakers |  |
| Cruise control/ speed limiter |  |
| **Safety and security** | Electronic Stability Program (ESP) |  |
| Anti-lock Braking System (ABS) |  |
| Electronic Brake-force Distribution (EBD) |  |
| Acceleration Skid Control (ASR) |  |
| Brake Assist  |  |
| Hill Assist functionality  |  |
| Three-point seat belts for all seats, ISOFIX mounting points for the 2nd and 3rd row of seats |  |
| Immobilizer |  |
| Front and lateral airbags (driver and passenger) |  |
| Engine and gearbox protection |  |
| Front and rear mud flaps  |  |
| **Accessories**  | First aid kit  |  |
| Powder fire extinguisher  |  |
| Car warning triangle  |  |
| Full-size spare wheel  |  |
| Full set of winter tyres on steel rims to complement the factory standard summer tyres |  |
| Car jack  |  |
| Tool kit, supplied by the manufacturer |  |
| 1 (one) additional key |  |