**ItB18/01752 - Annex 1 – Lot #1: Technical Responsiveness Table**

Bidders shall provide all the applicable data of the equipment offered, failing to do so may result in the bid being rejected. Corresponding documentation shall form part of the bidder’s offer.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Item Description** | **Specifications** | **√****Yes** | **√****No** | **Technical Compliance** **Please provide details /description of offered feature)**  |

|  |
| --- |
| **LOT #1** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  |  |  |  |
| **Product name** | **Waste plastic bin 120 lt**Mobile plastic container for waste with 2 wheels, lifting appliances with fork |  |  |  |
| **Destination** | -waste collection and recycling-Waste bin with 2 wheels adapted for standard handling and lifting device, stable to ultraviolet radiation, rectangular section, flat hinge cover |  |  |  |
| **Product certification** | - tested according to EN 840 -1:2013, EN 840 -5:2013, EN 840 -6:2013 |  |  |  |
| **System certifications** | Produced in integrated quality management system according to ISO 9001, ISO 14001 |  |  |  |
| **Volume, nominal** | 120 liters |  |  |  |
| **Payload** | 60 kg |  |  |  |
| **Weight, kg** | Not less than 8,5  |  |  |  |
| **Material** | High density polyethylene HDPE, free of heavy metals, UV resistant |  |  |  |
| **Color** | Black |  |  |  |
| **Body** | Square section |  |  |  |
| Flaps-flat, adapted to the body,mounted in 2 points to the body with 2 screw pins, 2 handles |  |  |  |
| 2 rubber wheels of 200 mm diameter, anti-corrosive, static load treated over 100 kg, 1 (one) galvanized solid metal axle |  |  |  |
| Frontal grip |  |  |  |
| Resistant handles, designed on the lid for a comfortable grip |  |  |  |
| Hinges assured |  |  |  |
| **Dimensions, mm (± 5%)** | Width – 480 |  |  |  |
| Length max. – 550 |  |  |  |
| Total height – 1000 |  |  |  |
| **Special construction****elements** | - 6 mm ribs for extra reinforcements on the upper part of the waste bin-wheels with solid rubber |  |  |  |
|  |  |

**See below table for the Lot #2**

**ItB18/01752 - Annex 1 – Lot #2 : Technical Responsiveness Table**

Bidders shall provide all the applicable data of the equipment offered, failing to do so may result in the bid being rejected. Corresponding documentation shall form part of the bidder’s offer.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Item Description** | **Specifications** | **√****Yes** | **√****No** | **Technical Compliance** **Please provide details /description of offered feature)**  |

|  |
| --- |
| **LOT #2** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  |  |  |  |
| **Product name** | Metallic waste container |  |  |  |
| **Destination** | Containers suitable for collection of home and industrial wastes |  |  |  |
| **Product certification** | DIN EN 840-3 and DIN EN 840-6 |  |  |  |
| **Volume, nominal** | 1100 liters |  |  |  |
| **Weight, kg** | 125 |  |  |  |
| **Body** | Hot dip galvanized |  |  |  |
| Lid - Hot dip galvanized Dome lidwith opening device for trunnion lifting systemLid opening and locking in 2 positions |  |  |  |
| Cover-hand-protection from profile-rubber(finger guard according to DIN EN-840-6) |  |  |  |
| Water outlet plug |  |  |  |
| Handles for easy movement |  |  |  |
| **Wheels** | Solid wheels with pivoting on 360° |  |  |  |
| 2 wheels Ø 200mm with brakes |  |  |  |
| 2 wheels Ø 200mm with directional stoppers |  |  |  |
| **Dimensions, mm (± 5%)** | A: Total height – 1415;B: Width – 1370;C: Length – 1030;D: Throw height – 1165;E: Wheel diameter – 200. |  |  |  |
|  |  |

All other information that we have not provided automatically implies our full compliance with the requirements, terms and conditions of the RFQ.

*[Name and Signature of the Supplier’s Authorized Person]*

*[Designation] \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ [Date]*