**Annex 4**

**Technical Compliance Table**

|  |  |  |
| --- | --- | --- |
| **Item** | **Description/Minimum specifications** | **Compliance**  **Yes/No**  ***(provide details)*** |
| **LOT I** | | |
|  | **Ballistic shield, type 1** |  |
| **1** | Handheld ballistic shield with additional leg protection (similar to the model in Annex 1a, **for illustration purpose only**) |  |
| Main shield:   * Dimensions: 600x1000 mm; * Ballistic protection level – NIJ Standard 01.08.01 for ballistic resistant protective materials, level IV (armor-piercing rifle) |  |
| Additional leg protection:   * Dimensions: 500x1000 mm; * Ballistic protection level – NIJ Standard 01.08.01 for ballistic resistant protective materials, level III-A (44 Magnum; Submachine Gun 9 mm) |  |
| Viewport (300x100 mm) with NIJ Level IV ballistic protection level |  |
| LED lighting system with strobe function and remote switch capability, mounted in the lower central region of the shield |  |
| Ambidextrous handle |  |
| High density foam padding beneath handle |  |
| Harness system for ballistic shield (similar to the model in Annex 1b, **for illustration purpose only**) |  |
| Black finish, inscription “Poliția” |  |
| **LOT II** | | |
|  | **Ballistic shield, type 2** |  |
| **2** | Handheld ballistic shield |  |
| Dimensions: 600x1000 mm |  |
| Ballistic protection level – NIJ Standard 01.08.01 for ballistic resistant protective materials, level III (High-Powered Rifle) |  |
| Viewport (300x100 mm) with NIJ Level III ballistic protection level |  |
| LED lighting system with strobe function and remote switch capability, mounted in the lower central region of the shield |  |
| Ambidextrous handle |  |
| High density foam padding beneath handle |  |
| Harness system for ballistic shield (similar to the model in Annex 1b, **for illustration purpose only**) |  |
| Black finish, inscription “Poliția” |  |
| **LOT III** | | |
|  | **Ballistic shield, type 3** |  |
| **3** | Small handheld ballistic shield |  |
| Ballistic protection level – NIJ Standard 01.08.01 for ballistic resistant protective materials, level III-A (44 Magnum; Submachine Gun 9 mm) |  |
| Dimensions: 600x500 mm |  |
| Ambidextrous handle |  |
| Ambidextrous weapon mount platform |  |
| High density foam padding beneath handle |  |
| Black finish, inscription “Poliția” |  |