**Annex 4**

**Technical Compliance Table**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Items to be Supplied\*** | **Quantity** | **Description / Specifications of Goods** | | | **Compliance**  **Yes/No**  *(provide details)* | |
| **Crew Van**  To be retrofitted with additional equipment and storage systems and used by the Anticorruption Center for their daily operation | **1** | **Body** | Standard non-metallic white colour |  | |
| Metallic structure divided virtually into three compartments (cab, passenger compartment and load compartment) |  | |
| **Year of manufacture** | 2018-2019; brand new vehicle |  | |
| **Steering** | Left-hand drive |  | |
| **Engine** |  |  | |
| *Displacement* | At least 1800 cm3 |  | |
| *Power* | At least 140 HP |  | |
| *Emission standard* | EURO 6 |  | |
| *Fuel type* | Diesel |  | |
| **Tank capacity** | At least 70 l |  | |
| **Seating** |  |  | |
| *Number and type of seats* | * 1 (one) driver`s seat with angle-adjustable armrest, adjustable head restraint and adjustable seat cushion angle; * 1 (one) two-passenger front bench with adjustable head restraints. |  | |
| *Upholstery* | High resistant dark fabric/cloth |  | |
| **Interior equipment** | Climate Control |  | |
| Non-slip floor covering |  | |
| **Dimensions** |  |  | |
| *Wheelbase* | At least 3500 mm |  | |
| *Overall length* | At least 6500 mm |  | |
| *Overall width (excl. door mirrors)* | Up to 2600 mm |  | |
| *Overall height* | At least 2000 mm |  | |
| *Load area height* | At least 1900 mm |  | |
| *Gross vehicle weight* | At least 3000 kg |  | |
| *Payload* | At least 1100 kg |  | |
| *Turning circle* | Up to 16 m |  | |
| **Electronics** | Alternator (12V/180 A) |  | |
| High capacity battery (minimum 90 Ah) |  | |
| Remote central locking |  | |
| Automatic headlights and wipers |  | |
| Electrically operated front windows |  | |
| Electrically adjustable/heated side view mirrors |  | |
| Front fog lamps |  | |
| Parking aid system (rear) |  | |
| Working lights in load/passenger compartments with accessible switch |  | |
| Interior door contact light over the rear door |  | |
| Metric instrument cluster (including at least speedometer, tachometer, odometer, fuel gauge, seat belt warning light, clock, outside temperature display) |  | |
| 12V power socket |  | |
| Audio device with AM/FM radio tuner, USB interface, speakers |  | |
| Van wiring should be able to support high charges following subsequent retrofitting (warning lights, electric car winch etc.) |  | |
| **Safety and security** | European New Car Assessment Programme (Euro NCAP) |  | |
| Electronic Stability Program (ESP) |  | |
| Anti-lock Braking System (ABS), |  | |
| Electronic Brake-force Distribution (EBD) |  | |
| Acceleration Skid Control (ASR) |  | |
| Brake Assist |  | |
| Three-point seat belts for driver seat and front bench |  | |
| Immobilizer |  | |
| Front airbags (driver and passenger) |  | |
| Engine and gearbox protection |  | |
| **Accessories** | First aid kit |  | |
| Powder fire extinguisher: 5 kg, stored in the rear compartment, with mounting devices |  | |
| Car warning triangle |  | |
| Full-size spare wheel |  | |
| Front and rear mudflaps |  | |
| Full set of winter tyres with steel rims to complement factory standard summer tyres |  | |
| Hydraulic jack |  | |
| Tool kit, supplied by the manufacturer |  | |
| Road hazard lamp |  | |
| 1 (one) additional key |  | |