**Annex 4**

**Technical Compliance Table**

|  |  |  |  |
| --- | --- | --- | --- |
| **Items to be Supplied\*** | **Quantity** | **Description / Specifications of Goods** | **Compliance** **Yes/No***(provide details)* |
| **Crew Van** To be retrofitted with additional equipment and storage systems and used by the Anticorruption Center for their daily operation | **1** | **Body** | Standard non-metallic white colour |  |
| Metallic structure divided virtually into three compartments (cab, passenger compartment and load compartment)  |  |
| **Year of manufacture** | 2018-2019; brand new vehicle |  |
| **Steering** | Left-hand drive |  |
| **Engine** |  |  |
| *Displacement*  | At least 1800 cm3 |  |
| *Power*  | At least 140 HP  |  |
| *Emission standard*  | EURO 6 |  |
| *Fuel type* | Diesel  |  |
| **Tank capacity**  | At least 70 l |  |
| **Seating** |  |  |
| *Number and type of seats*  | * 1 (one) driver`s seat with angle-adjustable armrest, adjustable head restraint and adjustable seat cushion angle;
* 1 (one) two-passenger front bench with adjustable head restraints.
 |  |
| *Upholstery*  | High resistant dark fabric/cloth  |  |
| **Interior equipment** | Climate Control  |  |
| Non-slip floor covering  |  |
| **Dimensions** |  |  |
| *Wheelbase*  | At least 3500 mm  |  |
| *Overall length*  | At least 6500 mm  |  |
| *Overall width (excl. door mirrors)* | Up to 2600 mm |  |
| *Overall height*  | At least 2000 mm |  |
| *Load area height* | At least 1900 mm  |  |
| *Gross vehicle weight*  | At least 3000 kg  |  |
| *Payload*  | At least 1100 kg  |  |
| *Turning circle* | Up to 16 m |  |
| **Electronics** | Alternator (12V/180 A)  |  |
| High capacity battery (minimum 90 Ah) |  |
| Remote central locking  |  |
| Automatic headlights and wipers |  |
| Electrically operated front windows |  |
| Electrically adjustable/heated side view mirrors |  |
| Front fog lamps  |  |
| Parking aid system (rear) |  |
| Working lights in load/passenger compartments with accessible switch  |  |
| Interior door contact light over the rear door |  |
| Metric instrument cluster (including at least speedometer, tachometer, odometer, fuel gauge, seat belt warning light, clock, outside temperature display) |  |
| 12V power socket  |  |
| Audio device with AM/FM radio tuner, USB interface, speakers |  |
| Van wiring should be able to support high charges following subsequent retrofitting (warning lights, electric car winch etc.) |  |
| **Safety and security** | European New Car Assessment Programme (Euro NCAP)  |  |
| Electronic Stability Program (ESP) |  |
| Anti-lock Braking System (ABS),  |  |
| Electronic Brake-force Distribution (EBD) |  |
| Acceleration Skid Control (ASR) |  |
| Brake Assist  |  |
| Three-point seat belts for driver seat and front bench  |  |
| Immobilizer |  |
| Front airbags (driver and passenger) |  |
| Engine and gearbox protection |  |
| **Accessories** | First aid kit  |  |
| Powder fire extinguisher: 5 kg, stored in the rear compartment, with mounting devices |  |
| Car warning triangle  |  |
| Full-size spare wheel  |  |
| Front and rear mudflaps |  |
| Full set of winter tyres with steel rims to complement factory standard summer tyres |  |
| Hydraulic jack  |  |
| Tool kit, supplied by the manufacturer |  |
| Road hazard lamp  |  |
| 1 (one) additional key |  |