Author: Dumitru
Last saved by: Natalia Volcovschi

Accessibility of the Entrance to the Ministry of Defense Building

Form No.1
WinCmeta

(name of the facility) |

List of Quantities of Works No. 35-01/2019

Crt. No. | Rule symbol and resource code | Name of works | Unit | Volume | BoQ value, MDL
| | | | | Per unit of measure ———— incl. salary | Total ——— incl. salary

1 | 2 | 3 | 4 | 5 | 6 | 7
| | Chapter 1. Outer Ramp | | | |
1 | TsA02E | Manual excavation of soil in limited spaces, less than 1.00 m or more than 1.00 m wide, executed without supports, with vertical slope, at foundations, canals, basements, drains, steps, in medium or very cohesive soil <1.5 m deep, average soil | m3 | 8.8000 | |
2 | TsD01B | Spreading loose soil from a heap with a shovel at a distance of up to 3 m in uniform layers 10-30 cm in thickness, breaking up clods, average soil | m3 | 8.8000 | |
3 | TsD04B | Manual punning of landfill executed in horizontal or 1/4 inclined excavations, including watering of each layer of soil separately, 10 cm in thickness, cohesive soil | m3 | 8.8000 | |
4 | CA03A2 | Pouring of concrete into foundations, plinths, supporting walls, walls below zero mark, prepared with concrete mixer on site and pouring with classical means, simple concrete of grade C 5/4 (Bc 5/B 75) | m3 | 0.9600 | |
5 | CB02A | Formwork made from recycled panels with coating of short and shortened coniferous planks for poring concrete in foundation pads, socket-type footings and foundations for equipment, including fasteners | m2 | 44.0000 | |
6 | CC01E | OB 37 concrete reinforcement molded in site workshops and mounted with bars up to 8 mm in diameter, including continuous foundations and timbering | kg | 35.0000 | |
7 | CC01F1 | PC 52 concrete reinforcement molded in site workshops and mounted with bars over 8 mm in diameter, including continuous foundations and timbering | kg | 617.0000 | |
8 | CA03C2 | Pouring of concrete into foundations, plinths, supporting walls, walls below zero mark, prepared with concrete mixer on site and pouring with classical means, reinforced concrete of grade C 10/8 (Bc 10/B 150) | m3 | 7.7000 | |
9 | TsC53A | Compaction of soil with gravel | 100m2 | 0.0900 | |
10 | CA02A2 | Pouring of simple concrete for leveling, slopes, protective screeds up to 35 m high, preparation with concrete mixer on site and pouring with classical means, concrete of grade C 5/4 (Bc 5/B 75) | m3 | 0.9000 | |
11 | CC03A | Reinforcing fabric installation at height less than or equal to 35 m, on walls and diaphragms, fabric weight is up to 3 kg/sqm | kg | 20.1600 | |
12 | CA02B2 | Pouring of simple concrete for leveling, slopes, protective screeds up to 35 m high, preparation with concrete mixer on site and pouring with classical means, concrete of grade C 10/8 (Bc 10/B 150) | m3 | 1.3500 | |
13 | CC03A | Reinforcing fabric installation at height less than or equal to 35 m, on walls and diaphragms, fabric weight is up to 3 kg/sqm (fabric under granite) | kg | 36.3000 | |
14 | CG19A1 | Marble floors, ready molded and finished, 5 cm in thickness, mounted simply or according to the drawing, including 3 cm support layer of cement mortar M 100-T, including jointing with white cement, cleaning and washing with water, executed in rooms with areas less than or equal to 16 sqm, with strips | m2 | 17.0000 | |
15 | CK26D | Mounting the profile for rubber stairs | m | 36.0000 | |
16 | CI11A | Granite plywood applied on flat surfaces to walls and poles excluding the installation of esconsons, fixed with steel studs and cement mortar M 100-T with addition of lime 3 cm in thickness, grouted with white cement mortar and marble powder, respectively travertine, for tile sizes of up to 0.2 sqm/pc through (Thickness and color will be coordinated with the beneficiary) | m2 | 13.0000 | |
17 | CH06A calculation | Stainless steel metal handrail in 2 levels for people with disabilities 900 mm high, fixed on granite (Materials: stainless steel pipe 50*50 mm - 25 m.l, pipe for poles 30*50 - 26 m.l, round pipe 40 mm - 50 ml) | m | 24.6500 | |
| | Chapter 2. Hallway Ramp | | | |
18 | CH06A calculation | Stainless steel metal handrail in 2 levels for people with disabilities 900 mm high, fixed on granite (Materials: pipe for poles 30*50 - 19 m.l, round pipe 40 mm - 20 ml) | m | 10.0000 | |
19 | CL17A calculation | Stainless steel metal ware, apparently mounted: Rampant made of expanded sheet 5 mm in thickness, ready made | kg | 79.5000 | |

	                                                                                                         

(position, signature, surname, name)
L.S.