LIST OF QUANTITIES OF WORK
TO REQUEST THE PRICE OFFER

1. Name of the beneficiary: Ungheni town hall, Ungheni district   
2. The organizer of the procurement procedure: UNDP Moldova/ EU4Moldova: Focal Regions
3. The object of the procurement:  The reconstruction, arrangement and equipment of the UNGHENI INDUSTRIAL HUB
 
Bid currency: USD 

No
	Symbol of the norm and resource code	
Works and costs	
M.U.	Quantity as per project data	Estimated cost, USD	
					Per unit of measurement
	Total

1	2	3	4	5	6	7	
 		1. Floors (50% of level 4)
					
1	TsC54A	Sand foundation layer	m3	34,2000
			
 2	CG01A	Support layer for floors made of cement mortar M 100-T 3 cm thick with a finely chipped surface
	m2	1 142,0000
			
 3	CG01A1 k=4	Support layer for floors made of M 100-T cement mortar 3 cm thick with a finely chipped face. The difference in plus or minus for every 0.5 cm of M 100-T mortar support layer is added or subtracted
	m2	1 142,0000
			
 4	CG17D	Floors made of ceramic tiles including the support layer of adhesive mortar, executed on surfaces: larger than 16 m2
	m2	1 142,0000
			
 5	CG18A	Horizontal plinths with a maximum height of 15 cm on ceramic tile walls fixed with M 100-T cement mortar, including cleaning and washing with water, in rooms with surfaces larger than 16 square meters
	m	456,0000

		Total	 USD				
		Total Floors (50% of level 4)
Including salary					
		2. Finishing walls and pillars
					
6	CF54B	Cladding the walls with plasterboard boards, 12.5 mm thick, mounted on the galvanized profile structure: on flat surfaces, including door and window frames
	m2	282,0000
			
 7	CN53A	Priming the interior surfaces of the walls and ceilings
	m2	288,6000
			
 8	CF50B	Interior plasters of 5 mm thickness, executed by hand, with a dry mixture based on plaster, on walls and partitions, manual preparation of the mortar.
	m2	288,6000
			
 9	CN53A	Priming the interior surfaces of the walls and ceilings
	m2	570,6000
			
 10	CN06A	Interior painters with paint based on vinyl copolymers in aqueous emulsion, applied in 2 layers on the existing screed, executed by hand.
	m2	570,6000

		Total	USD				
		Total Finishing walls and pillars
Including salary					
		3. Finishing ceilings
					
11	CN53A	Priming the interior surfaces of the walls and ceilings
	m2	1 382,0000
			
 12	CN06A	Interior painters with paint based on vinyl copolymers in aqueous emulsion, applied in 2 layers on the existing screed, executed by hand.
	m2	1 382,0000
			
 13	CB14C	Tubular metal scaffold for finishing work on ceilings at heights up to 7 m, with scaffold immobilization for 15 days (120 hours)	m2	1 382,0000

		Total	USD				
		Total Finishing ceilings
Including salary					
		4. Separating walls
					
14	CD72H	Flat partitions made of plasterboard 75-125 mm thick on a simple metal frame with plasterboard in one layer on both sides with insulation, with a height of over 4 m
	m2	915,0000
			
 15	CN53A	Priming the interior surfaces of the walls and ceilings
	m2	1 830,0000
			
16	CF50B	Interior plastering with a thickness of 5 mm, manually executed using a dry mix based on gypsum, for walls and partitions	m2	915,0000

		Total	 USD				
		Total Separating walls
Including salary					
		5. Sewage, internal aqueduct
					
17	RpCU05I	Making holes for pipes or tie rods in stone or reinforced concrete walls of 26 - 50 cm
	buc	8,0000
			
 18	SB08E	Plastic pipe for sewerage, joined with a rubber gasket, mounted apparently or buried under the floor, having a diameter of 110 mm
	m	54,0000
			
19	SB09E	Plastic connecting piece for drainage, combined with a rubber gasket, with a diameter of 110 mm	buc	8,000			
20	SB08C	Plastic pipe for sewerage, joined with a rubber gasket, mounted apparently or buried under the floor, having a diameter of 50 mm
	m	52,0000
			
21	SB09C	Plastic connecting piece for drainage, combined with a rubber gasket, with a diameter of 50 mm	buc	11,0000			
22	SC07A1	Toilet bowl, fully equipped, made of semi-porcelain, sanitary porcelain, etc. including for the disabled, placed on the floor, with the water tank mounted on the vessel, at height or half height, having the internal siphon type S
	unit	18,0000
			
 23	SC04C	Semi-porcelain sink, sanitary porcelain, etc. including for the disabled, having a drain pipe made of plastic material, mounted on a pedestal
	unit	10,0000
			
 24	SA15B	Plastic pipe joined by polyfusion welding, in connecting pipes, to sanitary objects, to residential and social-cultural objects, having a diameter of 20 mm
	m	54,0000
			
 25	SA15B	Plastic pipe joined by polyfusion welding, in connecting pipes, to sanitary objects, to residential and social-cultural objects, having a diameter of 25 mm
	m	60,0000
			
 26	SA37B	Bracelet for fixing water and gas supply pipes, made of steel or PVC, mounted by embedding, the pipes having a diameter of 3/4"
	unit	54,0000
			
 27	SD06A	Pass valve with socket and Dutch connection, for steel pipe, having a diameter of 3/8" - 1/2"
	unit	38,0000
			
 28	SD03A	Faucet for a sink or washing machine, regardless of the closing method, including for the disabled, having a diameter of 1/2"
	unit	10,0000

		Total	 USD				
		Total Sewage, internal aqueduct
Including salary					
		6. Parking, 300 sqm
					
29	CC03C	Installation of welded nets at heights less than or equal to 35 m, on slabs
	kg	240,0000
			
 30	CA04C	Concrete poured into slabs, beams, columns, prepared with a concrete batching plant and pouring with classical means reinforced concrete class C 20/16 (Bc 20/B 250), at heights up to 35 m inclusive
	m3	45,0000

		Total	 USD				
		Total Parking, 300 sqm
Including salary					
		7. 1st floor
					
31	CG01A	Support layer for floors made of cement mortar M 100-T 3 cm thick with a finely chipped surface
	m2	400,0000
			
 32	CG01A1 k=4	Support layer for floors made of M 100-T cement mortar 3 cm thick with a finely chipped face. The difference in plus or minus for every 0.5 cm of M 100-T mortar support layer is added or subtracted
	m2	400,0000
			
 33	CK13B1	Sliding or folding metal doors and gates in two leaves mounted in masonry of any kind, including the necessary accessories, with an area over 7 sqm (industrial sectional doors (mechanical with reducer) without pedestrian doors 3.5x3.8m - 2 pcs.)
	m2	26,6000
			
 34	CK23A	Plastic windows with one or more sashes in buildings with heights up to 35 m inclusive, with a frame area up to 1.00 m2 inclusive
	m2	12,0000

		Total	USD				
		Total 1st floor
Including salary					
		8. 2nd Floor
					
35	CG22A2	Plain concrete floors class C 10/8 (Bc 10/B 150) 10 cm thick, in a continuous field, screed, with the application of a 2 mm gap, cast in place, in rooms with an area of more than 16 square meters
	m2	1 008,0000
			
 36	CG01A	Support layer for floors made of cement mortar M 100-T 3 cm thick with a finely chipped surface
	m2	600,0000
			
 37	CG47D	Ceramic tile floors, including the backing layer of adhesives (dry mix), tile sizes: over 300 x 300 mm
	m2	20,0000
			
 38	CF50B	Interior plasters of 5 mm thickness, executed by hand, with a dry mixture based on plaster, on walls and partitions, manual preparation of the mortar.
	m2	30,0000
			
 39	CF57A	Manual application of "Eurofin" gypsum-based putty 1.0 mm thick on the surfaces of walls, columns and ceilings
	m2	30,0000
			
40	CN06A	Interior painters with paint based on vinyl copolymers in aqueous emulsion, applied in 2 layers on the existing screed, executed by hand.
	m2	30,0000
			
 41	CK25A	Doors made of plastic profiles, including the necessary fittings and accessories for doors mounted in masonry of any kind in constructions with a height of up to 35 m inclusive, in one leaf, with a frame surface of up to 7 m2 inclusive
	m2	30,0000
			
 42	CD72H	Flat partitions made of plasterboard 75-125 mm thick on a simple metal frame with plasterboard in one layer on both sides with insulation, with a height of over 4 m
	m2	112,8000
			
 43	CN53A	Priming the interior surfaces of the walls and ceilings
	m2	112,8000
			
44	CF50B	Interior plastering with a thickness of 5 mm, manually executed using a dry mix based on gypsum, for walls and partitions	m2	112,8000			
 45	CN06A	Interior painters with paint based on vinyl copolymers in aqueous emulsion, applied in 2 layers on the existing screed, executed by hand.
	m2	112,8000
			
 46	CI06C	Glazed, unglazed, matte or glossy flour plywood with boards of the same color and format with dimensions from 15 x 15 cm to 30 x 30 cm, executed on flat surfaces on walls and pillars, including the jambs and edges, with alternating joints, in rooms with an area of more than 10 square meters, fixed with glue for the installation of plywood
	m2	108,0000
			
 47	CD64B	Ordinary masonry from limestone blocks (12cm mortar) with M-25, M-50 mortar preparation in site conditions for walls over 4 m high
	m3	34,0000
			
 48	RpEF13A	Installation of 60 W lighting fixtures (Horoz LED Lantern Lighting Fixtures NEHIR-36 36 W LED 6400 K 220 - 240 V IP65)
	unit	50,0000
			
 49	RpEE03A	Installation of bipolar sockets, normal construction in bakelite or aminoplast, single, double, waterproof construction, sealed, metal sealed or similar, mounted buried under the plaster or apparently on wooden or plastic dowels (220V sockets)
	unit	30,0000
			
 50	RpEE03C	Installation of 25-63 A cast iron bipolar sockets, mounted on consoles or in boxes and panels (380 V socket)
	unit	30,0000
			
 51	RpED01A	Installation of cables for electricity, installed freely in trenches or on the bottom of canals, with a conductor section up to 16 mmp (VVGng cable – 3 * 2,5 mm2 with copper wires)	m	800,0000

		Total	USD				
		Total 2nd Floor
Including salary					

		Total	 USD				
		Social and health insurance	24 %				
		Shipping costs	%				
		Overhead costs	%				
		Total	 USD				
		Estimate profit	 %				
		Total	 				
		
Total estimate:
Including salary					

BIDDER		
                                       (position, signature, name, surname)	
Certified Estimating Professional		
                                      (position, signature, name, surname)