Annex 4: Technical Compliance Table LOT 1
	No
	Technical Specifications 
(TS)
	Bidder’s response

	
	
	Compliance with TS
	Technical Compliance
(indicate the technical specifications of the proposed items)
	Proposed product image

	Manufacturer’s name, model/product reference, Catalogue or product link

	
	
	Yes, we comply
	No, we do not comply (indicate discrepancies)
	
	
	

	LOT 1: Standard School Furniture 

	1 
	Student desk and chair 
Desk: 
· Individual school desk with shelf 
· Tabletop dimensions: 700x500 mm 
· Adjustable height: 640-790 mm (7 levels, 25 mm each) 
· Tabletop: 18 mm melamine chipboard, smooth with rounded corners 
· Tabletop Edges: Polyurethane with pen compartment 
· Under-desk shelf: Metal mesh, 96 mm below the tabletop 
· Bag Hooks: Two schoolbag hooks 
· Fixing: Hidden screws to metal profiles 
· Frame: Oval metal pipe, electrostatically painted, polymerized 
· Gaskets: Durable plastic, height-adjustable, floor protection 
· Color: Gray 
Chair: 
· Height-adjustable school chair 
· Overall height: 755-895mm 
· Overall width: 475-515mm 
· Seat width: 405-445 mm 
· Seat depth: 425-465 
· Backrest width: 380-420 mm 
· Backrest height: 355-395mm, hole for ease of use 
· Adjustable seat height: 400/420/440/460 mm 
· Material: Solid molded plastic, quality polypropylene, light texture, resistant to fine scratches 
· Corners: Rounded and smooth 
· Frame: Oval metal tube, electrostatically painted, polymerized 
· Gaskets: Durable plastic, floor protection 
· Color: Gray 
  
	 
	
	
	
	

	2 
	Metal office cabinet 
· Metal office cabinet with 4 doors, 2 drawers, digital locks 
· Height: 1850mm 
· Width: 900mm 
· Depth: 400mm 
· Material: Cold-rolled steel, min. 0.7 mm thick. 
· Configuration: 2 upper glass-paneled doors, 2 central drawers, 2 lower solid metal doors. 
· Shelves: Metal, min. 30 kg load capacity per shelf. 
· Drawers: Smooth-running sliding mechanisms. 
· Locks: Key-operated locks for doors and drawers. 
· Finish: Corrosion-resistant powder coating. 
· Fittings: Metal handles, protective feet and wall-anchoring provision. 
· Safety: Smooth edges; safety glass for upper doors. 
· Color:  white gray 

	 
	
	  
	
	

	3 
	Blackboard for classrooms 
· Length: 2000mm 
· Width: 1000mm  
· Writing surface: Vitreous/porcelain enameled steel, minimum thickness 0.4 mm, green or black, matt finish, magnetic. 
· Frame: Anodized aluminium or equivalent corrosion-resistant material; rounded/protected corners with no exposed sharp edges. 
· Accessories: Chalk tray/holder and complete wall-mounting system included. 
	 
	
	  
	
	

	4 
	Teacher's chair
· Seat/Backrest: Plywood, Plastic, Polyurethane foam 
· Upholstery: Fabric 
· Arms: nylon 
· Base: Plastic 
· Castors: Rubberized 
· Mechanism: Tilt (lifting-lowering free swing with fixation in vertical working position of the backrest and swing tension adjustment) 
· Leg Color: white 
· Overall Width: 640mm 
· Overall Depth: 580mm 
· Overall Height min./max.: 960-1060mm 
· Seat width: 500mm 
· Seat depth: 480mm 
· Seat Height min./max.: 480-580mm 
· Backrest height: 480mm 
· Maximum permissible load: 120 kg 
 
	 
	
	
	
	

	5 
	Shelving unit on wheels 
· KANSTRUP black castor shelf 
· Material: steel 
· Height: 790mm 
· Width: 470mm 
· Depth: 310mm 
	 
	
	
	
	





Annex 4: Technical Compliance Table LOT 2
	No
	Technical Specifications 
(TS)
	Bidder’s response

	
	
	Compliance with TS
	Technical Compliance
(indicate the technical specifications of the proposed items)

	
	
	Yes, we comply
	No, we do not comply (indicate discrepancies)
	

	LOT 2: Custom-Made School Furniture

	1 
	Teacher's desk
· Table with three drawers, one drawer with lock 
· Material: Egger chipboard 18mm or comparable material 
· Color: H3157 ST12, Vicenza Oak or equivalent 
· PAL Color: U750 ST9, Taupe Grey or equivalent 
· Height: 750mm 
· Width: 1300mm 
· Depth: 800mm 
· Adjustable leg M8 
· Material: metal, profile 30*30*2mm 
· Metal Elements Color: RAL 7044 

	 
	
	

	2 
	Adjustable presentation table
· Table with adjustable metal leg with electrical connection 
· Compact material HPL 12mm 
· Radius 50mm 
· Max. load capacity: 100 kg 
· ASD color 1086 B, cookies & cream or similar 
· Leg color: gray or white 
· Height adjustable mechanism UPGRADE LIGHT 
· Speed: 32mm/s 
· Power type: 100V-240V 
· Decibel: <50dB 
· Height adjustment range: 450mm 
· Height: 750-1200mm 
· Width: 1300mm 
· Depth: 800mm 

	 
	
	  

	3 
	Washbasin
· Overall dimensions (W × D × H): 700 × 500 × 925 mm 
· Cabinet material: 18mm chipboard, Egger or comparable material 
· Cabinet Color: H3157 ST12 
· Countertop material: 12mm compact HPL or artificial stone 
· Countertop color: 1086 B, cookies & cream or equivalent 
· Washbasin: Rectangular undercounter basin, SEREL Aldo or equivalent, 560 × 375 × 205 mm 
· Mixer tap: Stainless steel washbasin mixer, countertop-mounted 

	 
	
	  

	4 
	Protective sheet for walls and workbenches for the laboratory technician
· Material: 36mm chipboard, Egger or comparable material 
· Color: U750 ST9 or equivalent 
· Total length: 338.08 m2 
· Skirting included 
· Note: Exact dimensions must be verified on-site before production begins (Falesti, Republic of Moldova) 

	 
	
	

	5 
	Built-in shelves 
· Material: Egger chipboard 36mm or comparable material 
· Color: U750 ST9 or equivalent 
· Approx. dimensions: 1400x2500mm 
· Configuration: 4 horizontal mid shelves 
· Installation: built-in, securely fixed to the wall. 
· Note: Exact dimensions must be verified on-site before production begins (Falesti, Republic of Moldova) 

	 
	
	

	6
	Mobile sink for chemistry laboratory
· Mobile chemistry laboratory sink with two containers for waste and fresh water 
· Dimensions (H × W × D): 860 × 550 × 380 mm 
· Material: 304 stainless steel construction 
· Sink: round stainless steel basin, approx. 330 mm diameter 
· Water capacity: Two removable containers of 25-27 liters each. 
· Pumping system: Integrated foot-operated manual pump or rechargeable battery-powered electric pump, supplying water from the fresh-water canister to the faucet. 
· Casters with brakes 
· Accessories: Stainless steel faucet, soap dispenser and all components required for operation 
· Battery: optional 

	
	
	

	7
	Worktable with incorporated refrigerator for chemistry & biology laboratories

Worktable: 
· Worktable with three compartments, with a refrigerator 
· Material: 18mm chipboard, Egger or comparable material 
· Refrigerator compartment: Approx. 656 mm wide, with ventilation grille and adequate installation clearance. 
· Cabinet color: U750 ST9 or equivalent 
· Countertop color: H193 ST12 or equivalent 
· Height: 1200mm  
· Width: 1800mm 
· Depth: 600mm 
 Refrigerator with freezer:  
· Refrigerator capacity: 116 liters 
· Freezer capacity: 16 liters 
· Total capacity: 132 liters 
· LED lighting  
· Height: maximum 82cm 
· Width: maximum 60cm 
· Depth: maximum 57cm 
· Features: LED interior lighting and adjustable temperature control 

	
	
	

	8
	Wall-mounted coat rack panel with wooden hooks
· Panel Width 2,500 mm × Height 1,200 mm 
· Panel thickness: 18 mm 
· Panel material: White laminated plywood  
· Panel colour: White 
· Panel shape: Rectangular, with rounded corners 
· Corner radius: R60 mm 
· Hook material: Solid ash wood (frasin) 
· Hook diameter: 20 mm 
· Hook colours: Yellow, red and blue 
· Number of Hooks per panel unit: 64 hooks 
· Hook arrangement: fixing spacing of 100 mm 
· Hook projection: As indicated in the approved technical drawing, with secure concealed mechanical fixings 
· Mounting system: Concealed metal suspension rails for wall-mounted units, MESAN type 
· Mounting height: Bottom edge of panel 750 mm above finished floor level

	
	
	

	9
	High freestanding hallway table/counter 
· Overall length: 2,700 mm 
· Overall depth:460 mm 
· Overall height: 950 mm 
· Main material: Laminated particleboard (PAL) or equivalent 
· Material thickness: 36 mm 
· Material type: Egger or of similar quality 
· Color: H1710 ST10 or equivalent 
· Vertical support: Two side panels, 36 mm thick 
· Clear distance between side supports: 2,628 mm 
· Height below worktop: 914 mm 
	
	
	

	10
	Hallway sofa with backrest and metal support frame
· Overall height: 843 mm 
· Overall depth: 641 mm 
· Overall length: 1300mm 
· Seat height: Approximately 450 mm above floor, derived from the front elevation 
· Upholstery: Textile fabric 
· Upholstery colour: RAL 3016 or equivalent 
· Backrest: Upholstered, slightly inclined 
· Backrest height: 450 mm  
· Seat depth: 504 mm  
· Support frame: Welded metal square tubing 
· Metal profile: 25 × 25 × 2 mm 
· Metal frame colour: RAL 9004 or equivalent 
· Frame finish: Painted metal 
· Backrest and seat geometry: Inclination angles of 80°, 95° and 107° indicated in side elevation 

	
	
	

	11
	Trapezoidal Upholstered Bench with Metal Frame
· Overall length: 1,085 mm 
· Lower edge length: 810–815 mm, depending on orientation 
· Overall depth: 500 mm 
· Overall height: 450 mm 
· Shape: Asymmetrical trapezoidal seating surface 
· Upholstery material: Textile fabric suitable for public spaces 
· Upholstery colour: RAL 6011 or equivalent 
· Upholstery requirement: Wear-resistant fabric for public spaces, as indicated in drawing 
· Metal structure: Round metal tubing 
· Metal tube diameter: 30 mm 
· Metal frame colour: RAL 9004 or equivalent 
· Frame/leg height: 200 mm 
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