**Annex 2**

**FORM FOR SUBMITTING SUPPLIER’S QUOTATION**

***(This Form must be submitted only using the Supplier’s Official Letterhead/Stationery[[1]](#footnote-1))***

We, the undersigned, hereby accept in full the UNDP General Terms and Conditions, and hereby offer to supply the items listed below in conformity with the specification and requirements of UNDP as per RFQ Reference No. RfQ-17/01627 – Supply of Plastic waste bins - 120 liters (Lot #1) and Metallic waste containers - 1100 liters (Lot #2).

|  |
| --- |
| **LOT #1** |

**TABLE 1: Offer to Supply Equipment Compliant with Technical Specifications and Requirements**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Item No.** | **Description/Specification of equipment** | **Quantity** | **Latest Delivery Date** | **Unit Price** | **Total Price per Item** |
|  | **Waste plastic bin – 120 liters** | 1900 | 60 days |  |  |
|  | Add: Cost of Transportation **[[2]](#footnote-2)** | | | |  |
|  | Add: Cost of Insurance | | | |  |
|  | Add: Other Charges (pls. specify) | | | |  |
|  | **Total Final and All-Inclusive Price Quotation (USD, VAT 0%)** | | | |  |

**TABLE 3 : Offer to Comply with Other Conditions and Related Requirements**

|  |  |  |  |
| --- | --- | --- | --- |
| **Other Information pertaining to our Quotation are as follows:** | **Your Responses** | | |
| ***Yes, we will comply*** | ***No, we cannot comply*** | ***If you cannot comply, pls. indicate counter proposal*** |
| Delivery Lead Time (up to 60 calendar days from PO contract signature) |  |  |  |
| Warranty and Quality Requirements |  |  |  |
| 1. Minimum 12 months of warranty |  |  |  |
| 1. Availability of certificates of quality, conformity and origin for the offered equipment |  |  |  |
| Validity of Quotation: 60 calendar days |  |  |  |
| All Provisions of the UNDP General Terms and Conditions |  |  |  |

**(see other tables below)**

**TABLE 4 : Technical Responsiveness Table**

Bidders shall provide all the applicable data of the equipment offered, failing to do so may result in the bid being rejected. Corresponding documentation shall form part of the bidder’s offer.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Item Description** | **Specifications** | **√**  **Yes** | **√**  **No** | **Technical Compliance**  **Please provide details /description of offered feature)** |

|  |
| --- |
| **LOT #1** |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  | |  |  |  |
| **Product name** | **Waste plastic bin 120 lt**  Mobile plastic container for waste with 2 wheels, lifting appliances with fork |  |  |  |
| **Destination** | -waste collection and recycling  -Waste bin with 2 wheels adapted for standard handling and lifting device, stable to ultraviolet radiation, rectangular section, flat hinge cover |  |  |  |
| **Product certification** | - tested according to EN 840 -1:2013, EN 840 -5:2013, EN 840 -6:2013 |  |  |  |
| **System certifications** | Produced in integrated quality management system according to ISO 9001, ISO 14001 |  |  |  |
| **Volume, nominal** | 120 liters |  |  |  |
| **Payload** | 60 kg |  |  |  |
| **Weight, kg** | Not less than 8,5 |  |  |  |
| **Material** | High density polyethylene HDPE, free of heavy metals, UV resistant |  |  |  |
| **Color** | Black |  |  |  |
| **Body** | Square section |  |  |  |
| Flaps-flat, adapted to the body,  mounted in 2 points to the body with 2 screw pins, 2 handles |  |  |  |
| 2 rubber wheels of 200 mm diameter, anti-corrosive, static load treated over 100 kg, 1 (one) galvanized solid metal axle |  |  |  |
| Frontal grip |  |  |  |
| Resistant handles, designed on the lid for a comfortable grip |  |  |  |
| Hinges assured |  |  |  |
| **Dimensions, mm (± 5%)** | Width – 480 |  |  |  |
| Length max. – 550 |  |  |  |
| Total height – 1000 |  |  |  |
| **Special construction**  **elements** | - 6 mm ribs for extra reinforcements on the upper part of the waste bin  -wheels with solid rubber |  |  |  |
|  | |  | | |

**L**

|  |
| --- |
| **LOT #2** |

**TABLE 1: Offer to Supply Equipment Compliant with Technical Specifications and Requirements**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Item No.** | **Description/Specification of equipment** | **Quantity** | **Latest Delivery Date** | **Unit Price** | **Total Price per Item** |
|  | **Metallic waste container** | 134 | 60 days |  |  |
|  | Add: Cost of Transportation **[[3]](#footnote-3)** | | | |  |
|  | Add: Cost of Insurance | | | |  |
|  | Add: Other Charges (pls. specify) | | | |  |
|  | **Total Final and All-Inclusive Price Quotation (USD, VAT 0%)** | | | |  |

**TABLE 3 : Offer to Comply with Other Conditions and Related Requirements**

|  |  |  |  |
| --- | --- | --- | --- |
| **Other Information pertaining to our Quotation are as follows:** | **Your Responses** | | |
| ***Yes, we will comply*** | ***No, we cannot comply*** | ***If you cannot comply, pls. indicate counter proposal*** |
| Delivery Lead Time (up to 60 calendar days from PO contract signature) |  |  |  |
| Warranty and Quality Requirements |  |  |  |
| 1. Minimum 12 months of warranty |  |  |  |
| 1. Availability of certificates of quality, conformity and origin for the offered equipment |  |  |  |
| Validity of Quotation: 60 calendar days |  |  |  |
| All Provisions of the UNDP General Terms and Conditions |  |  |  |

**TABLE 4 : Technical Responsiveness Table**

Bidders shall provide all the applicable data of the equipment offered, failing to do so may result in the bid being rejected. Corresponding documentation shall form part of the bidder’s offer.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Item Description** | **Specifications** | **√**  **Yes** | **√**  **No** | **Technical Compliance**  **Please provide details /description of offered feature)** |

|  |
| --- |
| **LOT #2** |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  | |  |  |  |
| **Product name** | Metallic waste container |  |  |  |
| **Destination** | Containers suitable for collection of home and industrial wastes |  |  |  |
| **Product certification** | DIN EN 840-3 and DIN EN 840-6 |  |  |  |
| **Volume, nominal** | 1100 liters |  |  |  |
| **Weight, kg** | 125 |  |  |  |
| **Body** | Hot dip galvanized |  |  |  |
| Lid - Hot dip galvanized Dome lid  with opening device for trunnion lifting system  Lid opening and locking in 2 positions |  |  |  |
| Cover-hand-protection from profile-rubber  (finger guard according to DIN EN-840-6) |  |  |  |
| Water outlet plug |  |  |  |
| Handles for easy movement |  |  |  |
| **Wheels** | Solid wheels with pivoting on 360° |  |  |  |
| 2 wheels Ø 200mm with brakes |  |  |  |
| 2 wheels Ø 200mm with directional stoppers |  |  |  |
| **Dimensions, mm (± 5%)** | A: Total height – 1415;  B: Width – 1370;  C: Length – 1030;  D: Throw height – 1165;  E: Wheel diameter – 200. |  |  |  |
|  | |  | | |

All other information that we have not provided automatically implies our full compliance with the requirements, terms and conditions of the RFQ.

*[Name and Signature of the Supplier’s Authorized Person]*

*[Designation] \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ [Date]*

1. *Official Letterhead/Stationery must indicate contact details – addresses, email, phone and fax numbers – for verification purposes*  [↑](#footnote-ref-1)
2. *Pricing of goods should be consistent with the INCO Terms indicated in the RFQ* [↑](#footnote-ref-2)
3. *Pricing of goods should be consistent with the INCO Terms indicated in the RFQ* [↑](#footnote-ref-3)