Rehabilitation of aqueduct from the Nationala str. to Solidaritate str. in Ungheni city		
(name of the site)		

Bill of work quantities 

External aqueduct networks 		Offer currency USD
	
№
	Symbol of the norm and resource code  	
Name of works      	
U.M. 	Quantity  	Price per unit of measurement, USD
 salary	Total, 
USD
salary	

1	2	3	4	5	6	7	
		Chapter 1. Equipment/machinery 
					
1	Company prices
	 Cast iron fire hydrant with          D = 125mm mounted underground,  H=1.00m	piece	4			
 2	Company prices
	Cast iron fire hydrant with           D = 125mm mounted underground,  H=1.25m	piece	1			
 3	Company prices
	 Cast iron fire hydrant with          D = 125mm mounted underground ,  H=1.50m	piece	4			
 4	Company prices	Cast iron fire hydrant with           D = 100mm mounted underground,  H=2,00m	piece	1			
 5	Company prices
	Cast iron T-bend TФ300x100mm, 	piece	1			
 6	Company prices
	Cast iron T-bend ТФ 300х150 mm	piece	1			
 7	Company prices
	Straight cast iron T-bend with flanges   100 mm	piece	1			
 8	Company prices
	Straight cast iron T-bend with flanges   200 mm	piece	1			
 9	Company prices
	Straight cast iron T-bend with flanges   300 mm	piece	2			
 10	Company prices
	Straight cast iron T-bend with flanges   400 mm	piece	1			
 11	Company prices
	Enameled cast iron valve with rubberized wedge with fringes D300 mm, similar to HAWLE 	piece	5			
 12	Company prices
	Enameled cast iron valve with rubberized wedge with fringes D150  mm, similar to HAWLE 

	piece	3			
 13	Company prices

	Enameled cast iron valve with rubberized wedge with fringes D100 mm, similar to HAWLE 	piece	16			
 14	Company prices
	Enameled cast iron valve with rubberized wedge with fringes D200 mm,  similar to HAWLE 	piece	1			
 15	Company prices
	Enameled cast iron valve with rubberized wedge with fringes D50 mm, similar to HAWLE 	piece	6			
 16	Company prices
	Enameled cast iron valve with rubberized wedge with fringes D65mm, similar to HAWLE 	piece	1			
 17	Company prices
	Enameled cast iron valve with rubberized wedge with fringes D400 mm, similar to HAWLE 	piece	4			
 18	Company prices
	Flange head 400mm	piece	4			
 19	Company prices
	Flange head 315mm	piece	6			
 20	Company prices
	PE bend 90*   D315 mm	piece	1			
 21	Company prices
	PE bend 30*   D315 mm	piece	2			
 22	Company prices
	Cast iron adapter Sleeve-flange 300mm	piece	3			
 23	Company prices
	Cast iron adapter Sleeve-flange 400mm	piece	2			
 24	Company prices
	Cast iron adapter coupling XPФ 300x150 mm	piece	1			
 25	Company prices
	Cast iron adapter coupling XФ 110/50 mm	piece	2			
 26	Company prices
	Cast iron adapter coupling XФ 110/65 mm	piece	1			
 27	Company prices
	Connection saddle with emission Cast iron flange 400/100mm	piece	1			
 28	Company prices
	Connection saddle with emission Cast iron flange 300/32mm
	piece	2			
 29	Company prices
	Connection saddle with emission Cast iron flange 400/32mm
	piece	1			
 30	Company prices
	Connection saddle with emission Cast iron flange 400/50mm
	piece	5			
 31	Company prices	Cast iron double sleeve regulator 400mm	piece	5			
 32	Company prices	Support for hydrant 150mm	piece	1			
 33	Company prices
	Support for hydrant  100mm	piece	9			
 34	Company prices
	Hydrant indicator (photo-luminescent)	piece	10			
 35	Company prices
	Polyethylene bend 30* PE100 PN10 d400mm	piece	5			
 36	Company prices
	Polyethylene bend 15* PE100 PN10 d400mm	piece	4			
 37	Company prices
	Polyethylene bend 45* PE100 PN10 d400mm	piece	8			
 38	Company prices
	Polyethylene reduced T-bend with sleeves and emission with flange 400/100	piece	8			
 39	Company prices
	Polyethylene reduced T-bend with sleeves and emission with flange 400/150	piece	1			
 40	Company prices
	Polyethylene reduced T-bend with sleeves and emission with flange 400/200	piece	1			
  		Direct costs	 USD				
		Storage costs 	    - %				
		TOTAL Chapter 1.	USD				
		Including salary	USD				
 		Chapter 2. Assembling works 
					
41	AcB01A
	Assembling the manually or mechanically operated fittings (valves) on water supply pipes with diameter of 50-100 mm 	piece	23			
 42	AcB01B
	Assembling the manually or mechanically operated fittings (valves) on water supply and sewerage pipes with diameter of 125-150 mm  	piece	3			
 43	AcB01C
	Assembling the manually or mechanically operated fittings (valves) on water supply and sewerage pipes with diameter of 200-250 mm  	piece	1			
 44	AcB01D
	Assembling the manually or mechanically operated fittings (valves) on water supply and sewerage pipes with diameter of 300-400 mm 
	piece	6			
 45	AcB13A
	Manual handling (closing and opening) of ground mounted valves so as to isolate different zones in the network, the valves having the diameter of 50-200 mm 	piece	27			
 46	AcB13B
	Manual handling (closing and opening) of ground mounted valves so as to isolate different zones in the network, the valves having the diameter of 250-350 mm 	piece	5			
 47	AcB13C
	Manual handling (closing and opening) of ground mounted valves so as to isolate different zones in the network, the valves having the diameter of 400-500 mm 	piece	1			
  		Direct costs 	 USD				
		Social and health insurance	27.50 %				
		Total	100+				
		Overhead costs 	- %				
		Total	100+				
		Estimate benefit 	- %				
		TOTAL Chapter 2.	USD				
		Including salary	USD				
 		Chapter 3. Construction works 					
		Chapter 3.1. Earthworks 
					
48	TsC03B1
	Mechanic digging with excavator of 0.40-0.70 m3, with internal combustion engine and hydraulic command, in grounds with natural humidity, and unloading in the storage of ground cat. II
	100 m3	24,20			
 49	TsA20B
	Manual digging of soil, in breakers, with canal embankment dug with the excavator  or scraper for completing the cutting slopes, in middle ground (fine excavation)
	m3	74,87			
 50	TsA16B3
	Manual digging of soil, in limited spaces, in tranches up to 4 m depth, for electrical cables and other communication, in grounds with natural humidity and supporters 

	m3	726,80			
 51	Dl105
	Compacting ground of cat. II with mechanical knockers in depth of 0.6m	100 m3	10,05			
 52	TsF05B
	Supporting the banks with metal planks placed horizontally, in digging performed in limited spaces, with width up to 1.50 m between the banks and depth up to 4 m, interspaces between planks 0.21...0.60 m 	m2	4 479,90			
 53	TsC03F1
	Mechanic digging with excavator of 0.40-0.70 m3, with internal combustion engine and hydraulic command, in grounds with natural humidity, and unloading in motor cars of ground cat. II (digging and loading soil necessary for plugging)	100 m3	4,90			
 54	TsI50C
	Transporting the soil with trucks at a distance of 3 km 	t	834,05			
 55	TsC51B
	Unloading soil in storage, ground of category II	100 m3	4,91			
 56	TsD01B
	Spreading with the shovel of light soil in uniform layers, 10-30 cm thick, with a throw of up to 3 m of piles , including smashing of earth bolls from middle ground	m3	1 114,00			
 57	TsD04B
	Compacting with manual knocker of the embankments in horizontal of inclined digs to 1/4, including watering every layer of soil separately, with the thickness of 10 cm of cohesive ground	m3	1 602,87			
 58	TsD02B1
	Spreading the loose land coming from the fields of category I and II, executed with caterpillar tractor-based bulldozer 65-80 HP, in layers with thickness of 21-30 cm	100 m3	25,99			
 59	TsD05B
	Compacting with the mechanical knocker of 150-200 kg filling in the successive layers of 20-30 cm thickness, excluding the watering of every layer separately, the earth fillings being executed from non-cohesive ground
	100 m3	25,99			
		TOTAL, Chapter 3.1. Earthworks 
	USD				
		Including salary
	USD				
   		Chapter 3.2. Pipes and fittings 
					
60	AcA10D
	Fitting in the ground high density pressure polyethylene pipes, meant for water supply, assembled through butt-welding, according to standard I-6-PE, having the diameter of 400 mm, PE pipe for drinking water RC PE100PN10 SDR17
	m	1 324,00			
 61	AcA10C
	Fitting in the ground high density pressure polyethylene pipes, meant for water supply, assembled through butt-welding, according to standard I-6-PE, having the diameter of 315 mm, PE100 PN10 SDR17 RC
	m	329,00			

 63	AcA10B
	Fitting in the ground high density pressure polyethylene pipes, meant for water supply, assembled through butt-welding, according to standard I-6-PE, having the diameter of 160 mm  PE100 PN10, SDR17
	m	20,50			
 64	AcA10B
	Fitting in the ground high density pressure polyethylene pipes, meant for water supply, assembled through butt-welding, according to standard I-6-PE, having the diameter of 200 mm  PE100 PN10 SDR17
	m	5,00			
 65	AcA10A
	Fitting in the ground high density pressure polyethylene pipes, meant for water supply, assembled through butt-welding, according to standard I-6-PE, having the diameter of 110 mm  PE100 PN-10, SDR17 
	m	20,50			
 66	AcA52A
	Water supply polyethylene pipe mounted in ditch, with diameter of 63mm, РЕ 80; PN=10, SDR17
	m	16,50			
 67	AcA52A
	Water supply polyethylene pipe mounted in ditch, with diameter of 32 mm, РЕ 80; PN=10, SDR17
	m	6,00			
 68	GA08H
	Iron pipe protection tube, mounted in the ditch, when crossing the roads, for protection of the pipe, the tube having Dn 630 x 7 mm  
	m	58,50			
 69	GA08G
	Iron pipe protection tube, mounted in the ditch, when crossing the roads, for protection of the pipe, the tube having Dn 530 x 7 mm  
	m	26,50			
 70	AcB06B
	Installation of fire hydrants above the ground on existing positions, having the diameter Dn=125 mm (Installation of fire hydrants, H=1.0) 
	piece	3			
 71	AcB06B
	Installation of fire hydrants above the ground on existing positions, having the diameter Dn=125 mm (Installation of fire hydrants,  H=1.25) 	piece	1			
 72	AcB06B
	Installation of fire hydrants above the ground on existing positions, having the diameter Dn=125 mm (Installation of fire hydrants, H=1.5) 	piece	4			
 73	AcB06B
	Installation of fire hydrants above the ground on existing positions, having the diameter Dn=125 mm (Installation of fire hydrants, H=2) 	piece	1			
 74	AcA26C
	Coupling with flanges the linking pieces, flanges, including the blind flanges and fittings, with the diameter 300-400 mm (Cast iron T-bend 300/100)	piece	1			
 75	AcA26C
	Coupling with flanges the linking pieces, flanges, including the blind flanges and fittings, with the diameter 300-400 mm (Cast iron T-bend 300/150 mm)	piece	1			
 76	AcA26C
	Coupling with flanges the linking pieces, flanges, including the blind flanges and fittings, with the diameter 300-400 mm (Cast iron T-bend 300 mm)
	piece	2			
 77	AcA24C
	Coupling with flanges the linking pieces, flanges, including the blind flanges and fittings, with the diameter 300-400 mm (Cast iron T-bend 400 mm)	piece	1			
 78	AcA24B
	Coupling with sleeves the cast iron linking pieces or fittings, on pressure pipes, with diameter 125-250 mm (Cast iron T-bend 200 mm)
	piece	1			
 79	AcA24A
	Coupling with sleeves the cast iron linking pieces or fittings, on pressure pipes, with diameter 50-100 mm (Cast iron T-bend 100)
	piece	1			
 80	AcA26C
	Coupling with flanges the linking pieces, flanges, including the blind flanges and fittings, with the diameter 300-400 mm (Cast iron adapter coupling FM 300-400 mm)
	piece	1			
 81	AcA26B
	Coupling with flanges the linking pieces, flanges, including the blind flanges and fittings, with the diameter 125-250 mm (Cast iron adapter coupling 110/50 mm)
	piece	2			
 82	AcA26B
	Coupling with flanges the linking pieces, flanges, including the blind flanges and fittings, with the diameter 125-250 mm (Cast iron adapter coupling 110/65 mm)
	piece	1			
 83	AcA26C
	Coupling with flanges the linking pieces, flanges, including the blind flanges and fittings, with the diameter 300-400 mm (Connection saddle with emission Cast iron flange 400/100 mm)
	piece	1			
 84	AcA26C
	Coupling with flanges the linking pieces, flanges, including the blind flanges and fittings, with the diameter 300-400 mm (Connection saddle with emission Cast iron flange 300/32mm)
	piece	2			
 85	AcA26C
	Coupling with flanges the linking pieces, flanges, including the blind flanges and fittings, with the diameter 300-400 mm (Connection saddle with emission Cast iron flange 400/32mm)
	piece	1			
 86	AcA26C
	Coupling with flanges the linking pieces, flanges, including the blind flanges and fittings, with the diameter 300-400 mm (Connection saddle with emission Cast iron flange 400/50mm)
	piece	5			
 87	AcA26C
	Coupling with flanges the linking pieces, flanges, including the blind flanges and fittings, with the diameter 300-400 mm (Flange head 400mm)
	piece	4			
 88	AcA26C
	Coupling with flanges the linking pieces, flanges, including the blind flanges and fittings, with the diameter 300-400 mm (Flange head 315mm)

	piece	6			
 89	AcA26B
	Coupling with flanges the linking pieces, flanges, including the blind flanges and fittings, with the diameter 125-250 mm (Flange head D200)
	piece	1			
 90	AcA26B
	Coupling with flanges the linking pieces, flanges, including the blind flanges and fittings, with the diameter 125-250 mm (Flange head D160)
	piece	3			
 91	AcA26A
	Coupling with flanges the linking pieces, flanges, including the blind flanges and fittings, with the diameter 50-100 mm (Flange head 110 mm)
	piece	14			
 92	AcA24C
	Coupling with sleeves the cast iron linking pieces or fittings, on pressure pipes, with diameter 300-400 mm (Cast iron adapter Sleeve-flange D300 mm)
	piece	2			
 93	AcA24C
	Coupling with sleeves the cast iron linking pieces or fittings, on pressure pipes, with diameter 300-400 mm (Cast iron adapter Sleeve-flange D400 mm)	piece	2			
 94	AcA24C
	Coupling with sleeves the cast iron linking pieces or fittings, on pressure pipes, with diameter 300-400 mm 300-400 mm (Compensator with double sleeve of cast iron D400 mm)
	piece	5			
 95	AcB01A
	Installing manually or mechanically operated fittings (valves, taps, faucets) on the water supply or sewerage pipes, with diameter 50-100 mm (brass tap d25mm)
	piece	3			
 96	AcA54B
	Mechanic installation of fittings (screwing). Mechanic combination of the pipe and polyethylene fitting (sleeve, T-bend, bend), the pipes having the diameter of 50-110 mm.(Electro-fusion coupling with flange D63mm )
	piece	9			
 97	AcA54A
	Mechanic installation of fittings (screwing). Mechanic combination of the pipe and polyethylene fitting (sleeve, T-bend, bend), the pipes having the diameter of 20-40 mm. (Connection coupling 32mm)
	piece	4			
 98	AcA54B
	Mechanic installation of fittings (screwing). Mechanic combination of the pipe and polyethylene fitting (sleeve, T-bend, bend), the pipes having the diameter of 50-110 mm.( PE Benf 90* 315mm )
	piece	1			
 99	AcA54B
	Mechanic installation of fittings (screwing). Mechanic combination of the pipe and polyethylene fitting (sleeve, T-bend, bend), the pipes having the diameter of 50-110 mm.(PE Bend 30* 315mm )	piece	2			
 100	AcA53C
	Installing the fitting through electro-fusion. Electro-fusion welding type coupling between the pipe and the polyethylene fitting (sleeve, T-bend, bend), the pipes having the diameter of 110 mm. (Electro-fusion coupling with flange 75mm)	piece	1			
 101	AcA53A
	Installing the fitting through electro-fusion. Electro-fusion welding type coupling between the pipe and the polyethylene fitting (sleeve, T-bend, bend), the pipes having the diameter of 20, 25, 32, 40, 50, 63 mm. (Electro-fusion sleeve PE D63)	piece	3			
 102	GD53M
	Coupling through butt welding polyethylene fittings, with diameter of 400 mm, for adapters on flanges, domed lids, transition fittings and connection heads (and for the perpendicular branch of the T-bend) (PE bend 30*  PE100 PN10 d400mm)
	piece	5			
 103	GD53M
	Coupling through butt welding polyethylene fittings, with diameter of 400 mm, for adapters on flanges, domed lids, transition fittings and connection heads (and for the perpendicular branch of the T-bend) (PE bend 15*  PE100 PN10 d400mm)	piece	4			
 104	GD53M
	Coupling through butt welding polyethylene fittings, with diameter of 400 mm, for adapters on flanges, domed lids, transition fittings and connection heads (and for the perpendicular branch of the T-bend) (PE bend 45*  PE100 PN10 d400mm)
	piece	8			
 105	GD53M
	Coupling through butt welding polyethylene fittings, with diameter of 400 mm, for adapters on flanges, domed lids, transition fittings and connection heads (and for the perpendicular branch of the T-bend) (PE reduced T-bend with sleeves and emission with flange 400/100)
	piece	8			
 106	GD53M
	Coupling through butt welding polyethylene fittings, with diameter of 400 mm, for adapters on flanges, domed lids, transition fittings and connection heads (and for the perpendicular branch of the T-bend) (PE reduced T-bend with sleeves and emission with flange 400/150)
	piece	1			
 107	GD53M
	Coupling through butt welding polyethylene fittings, with diameter of 400 mm, for adapters on flanges, domed lids, transition fittings and connection heads (and for the perpendicular branch of the T-bend) (PE reduced T-bend with sleeves and emission with flange 400/200)
	piece	1			
 108	SA34I
	Manufacturing, fitting and cementing the protection tube for pipes crossing the manhole walls, having the diameter of 630mm L=0.2m
	piece	16			
 109	SA34I
	Manufacturing, fitting and cementing the protection tube for pipes crossing the manhole walls, having the diameter of 426.x7mm L=0.2m
	piece	7			
 110	SA34I
	Manufacturing, fitting and cementing the protection tube for pipes crossing the manhole walls, having the diameter of 219mm L=0.2m
	piece	3			
 111	SA34H
	Manufacturing, fitting and cementing the protection tube when pipes cross walls, with diameter 5" l=0.2 159mm	piece	12			
 112	SA34G
	Manufacturing, fitting and cementing the protection tube when pipes cross walls, with diameter 4" 108mm l=0.2m	piece	14			
 113	AcA31C
	Assembling though electrical welding the steel flanges, at the end of the pipes, having the diameter of 300 mm	piece	1			
 114	AcA31A
	Assembling though electrical welding the steel flanges, at the end of the pipes, having the diameter of 100 mm 	piece	3			
 115	AcA31B
	Assembling though electrical welding the steel flanges, at the end of the pipes, having the diameter of 150 mm 	piece	2			
 116	AcA31A
	Assembling through electrical welding the steel blind flange, at the end of the pipes, having the diameter of 100 mm 	piece	3			
 117	CL18A
	Support for pipes d315mm-27 pieces	kg	81,00			
 118	CL18A
	Support for pipes d400mm-24 pieces	kg	78,96			
 119	AcA26C
	Coupling with flanges the linking pieces, flanges, including blind flanges and fittings, having the diameter of 300 mm (coated steel free flange d400mm)
	piece	4			
 120	AcA26C
	Coupling with flanges the linking pieces, flanges, including blind flanges and fittings, having the diameter of 300 mm (free flange)
	piece	6			
 121	AcA26B
	Coupling with flanges the linking pieces, flanges, including blind flanges and fittings, having the diameter of 150 mm (free flange)
	piece	3			
 122	AcA26B
	Coupling with flanges the linking pieces, flanges, including blind flanges and fittings, having the diameter of 200 mm (free flange)
	piece	1			
 123	AcA26A
	Coupling with flanges the linking pieces, flanges, including blind flanges and fittings, having the diameter of 100 mm (free flange)
	piece	14			
 124	AcE51E
	Connection with the existing pipeline from steel pipes (with stub) with the diameter of the stub of 200 mm 
	piece	17			
 125	AcF11C
	Washing the  polyethylene pipes of 20-75 mm, for drinking water after installation and coupling, before reception 
	m	22,50			
 126	AcF11D
	Washing the  polyethylene pipes of 80-110 mm, for drinking water after installation and coupling, before reception
	m	20,50			
 127	AcF11E
	Washing   polyethylene pipes of 150-225 mm, for drinking water after installation and coupling, before reception  

	m	25,50			
 128	AcF11F
	Washing the  polyethylene pipes of 225 mm, for drinking water after installation and coupling, before reception  	m	1 653,00			
		TOTAL, Chapter 3.2
Pipes and fittings
	USD				
		Including salary	USD				
							
   		Chapter 3.3. Manholes, 
construction works 
					
129	AcD22B1
	Preparing and pouring concrete in the foundation of ditches, from internal side, with H 1.8-4 m and coverage 1-5 m, for concrete B10 procured from centralized stations (Concrete supporters made of concrete В20)
	m3	19,16			
 130	IzF04J1
	Hot-made waterproof layer for terraces, roofs or foundations and slabs, in fields without groundwater, including moldings and valleys from the current waterproofing protection: separation layer related to waterproofing works, executed with simple bitumen cardboard laid in unjointed overlaps (Supporters)
	m2	80,34			
 131	AcD53B
	Executing the manholes from precast reinforced concrete elements, for circular (ring-type) water supply, with diameter of 1.5 m, in grounds without underground water  
	m3	18,43			
 132	AcD53B1
	Precast reinforced concrete elements of manholes, for circular (ring-type) water supply, with diameter of 1.5 m, in grounds without underground water  
	piece	12			
 133	AcD53C
	Executing the manholes from precast reinforced concrete elements, for circular (ring-type) water supply, with diameter of 2.0 m, in grounds without underground water  

	m3	8,99			
 134	AcD53C1
	Precast reinforced concrete elements of manholes, for circular (ring-type) water supply, with diameter of 2.0 m, in grounds without underground water  
	well	4,00			
 135	AcD52A
	Executing the manholes from precast reinforced concrete elements, for circular (ring-type) water supply, with diameter of 1.0 m, in grounds without underground water  
	m3	6,15			
 136	AcD52A1
	Precast reinforced concrete elements of manholes, for circular (ring-type) water supply, with diameter of 1.0 m, in grounds without underground water  
	well	7			
 137	AcE07C
	Installing cast iron of cast iron- concrete hatches without the support piece for the manholes of water supply and sewerage installations, carriageway type III A and B 
	piece	23			
 138	AcE09A
	Assembling steel-concrete stairs with D=20 mm, for the manholes, made of masonry, concrete or clinker blocks 
	piece	161			
 139	DA06A1
	Layer of cylindered natural aggregates, having the function of filtering, insulation, ventilation, anti-freezing and anti-capillary resistance, with ballast-based manual coverage (Paving)
	m3	8,60			
 140	DE12C
	Asphalt poured on roadsides, on existing foundation, 3.0 cm. thickness (Paving)
	m2	41,80			
 141	CN01A
	Simple painting based on lime water, executed internally or externally on any surface, supported by two layers of lime water 	m2	135,00			
		TOTAL, Chapter 3.3.
Manholes, 
construction works 	USD				
		Including salary	USD				
							
   		Chapter 3.4. Demolishing and refurbishing parts of carriageway and roadsides 					
142	DC04B
	Cutting with machine having diamond disks the contraction and expansions joints in the old concrete on the carriageway and roadsides 
	m	1 947,00			
 143	Dl109
	Mechanized scouring of asphaltic concrete carpet and concrete slabs on the carriageway and roadsides 
	m3	83,03			
 144	Dl118
	Mechanized scouring of gravel + sand carpet on the carriageway and roadsides 	m3	178,79			
 145	TsC03H1
	Mechanic digging with excavator of 0,40-0,70 m3, with internal combustion engine and hydraulic command, in grounds with natural humidity, and unloading in motor-cars, ground category  IV 	100 m3	1,72			
 146	TsI50C
	Transportation of loads with the trucks at a distance of 3 km 	t	216,55			
 147	TsC51C
	Unloading soil in storages, ground category III 	100 m3	1,72			
 148	TsC54B
	Foundation layer of crushed stone 	m3	71,32			
 149	TsC54A
	Foundation layer of sand 	m3	107,47			
 150	DB16H k=1.5
	Asphalt concrete covering with small aggregates, executed in hot conditions, in thickness of 6.0 cm, with mechanical laying (carriageway)	m2	475,50			
 151	DB19F k=1.6
	Asphalt concrete covering with big aggregates, executed in hot conditions, in thickness of 8.0 cm, with mechanical laying (carriageway)	m2	475,50			
 152	DB20C
	Asphalt poured on the carriageway, in thickness of 5.0 cm, with manual laying (roadside)	m2	216,50			
 153	DI20A
	Preparing the cement concrete and fluidized cement concrete covering, made in fixed stations, compression with vibrating plates M200 (roadside)	m3	5,63			
 154	DG04B
	Disassembling stone or concrete borders of any size, laid on concrete 	m	168,00			
 155	DE10A
	Precast concrete borders for roadsides 20x25 cm, on concrete foundation 30x15 cm (recovery 80%)	m	168,00			
 156	TsE01B
	Manual levelling of fields and platforms with bumps of 10-20 cm, in middle ground 	100m2	7,53			
 157	TsH09A
	Sowing lawns on horizontal surfaces or in slopes of 30%
	100m2	7,53			
    		TOTAL, Chapter 3.4 Demolishing and refurbishing parts of carriageway and roadsides	 USD				
		Including salary	USD				
		Direct cost
	USD				
		Transportation of materials 	- %				
		Storage expenses	- %				
		Social and health insurance 	27.50 %				
		Total	100.00 +				
		Topographic control survey in DVG format and on drawings	USD				
		Overhead costs 	- %				
		Total	100.00 +				
		Estimate benefit 	- %				
 
	Total:					
	Total estimate:					

Note: The Bidder's costs will include all expenses including: materials and / or equipment, salaries, social payments, indirect expenses

Bidder____________________________________________________________________
(position, signature, name, surname)