## **ANNEX 3: TECHNICAL AND FINANCIAL OFFER - GOODS**

*Bidders are requested to complete this form, sign it and return it as part of their bid along with Annex 2: Quotation Submission Form. The Bidder shall fill in this form in accordance with the instructions indicated. No alterations to its format shall be permitted and no substitutions shall be accepted.*

|  |  |  |
| --- | --- | --- |
| Name of Bidder: | Click or tap here to enter text. | |
| RFQ reference: | **RfQ21/02304: EU4MD/ Supply of Plastic waste bins – 120 liters (Lot #1), 240 liters (Lot #2) and 1100 liters (Lot #3)** | Date: Click or tap to enter a date. |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **LOT #1** | | | | | | |
| **Currency of the Quotation: MDL Moldovan Lei**  **INCOTERMS: DAP** | | | | | | |
| **Item No** | **Description** | | **UOM** | **Qty** | **Unit price** | **Total price** |
| **1** | **Waste plastic bin 120 liters**  Mobile plastic containers for waste with 2 wheels, lifting appliances with fork | | **unit** | **200** |  |  |
| **Destination** | - waste collection and recycling  - waste bin with 2 wheels adapted for standard handling and lifting device, stable to ultraviolet radiation, rectangular section, flat hinge cover |
| **Product certification** | Tested according to EN 840 – 1:2013, EN 840 – 5:2013, EN 840 – 6:2013 |
| **System certification** | Produced in integration quality management system according to ISO 9001, ISO 14001 |
| **Volume, nominal** | 120 liters |
| **Weight, kg (min)** | 7 kg |
| **Material** | High density polyethylene HDPE, free of heavy metals, UV resistant |
| **Color** | Blue |
| **Body** | Square section  Flaps-flat, adapted to the body,  Mounted in 2 points to the body with 2 screw pins, 2 handles  2 rubber wheels of 200 mm diameter, anti-corrosive, static load treated over 100 kg, 1 (one) galvanized solid metal axe  Frontal grip  Resistance handle, designed on the lid for a comfortable grip  Hinges assured |
| **Dimensions, mm (±5%)** | Width max. – 480  Length max. – 550  Height max. - 1000 |
| **Special construction element** | 6 mm ribs extra enforcement on the upper part of the waste bin  wheels with solid rubber  strong bottom |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **LOT #2** | | | | | | |
| **Currency of the Quotation: MDL Moldovan Lei**  **INCOTERMS: DAP** | | | | | | |
| **Item No** | **Description** | | **UOM** | **Qty** | **Unit price** | **Total price** |
| **1** | **Waste plastic bin 240 liters**  Mobile plastic containers for waste with 2 wheels, lifting appliances with fork | | **unit** | **100** |  |  |
| **Destination** | - waste collection and recycling  - waste bin with 2 wheels adapted for standard handling and lifting device, stable to ultraviolet radiation, rectangular section, flat hinge cover |
| **Product certification** | Tested according to EN 840 – 1:2013, EN 840 – 5:2013, EN 840 – 6:2013 |
| **System certification** | Produced in integration quality management system according to ISO 9001, ISO 14001 |
| **Volume, nominal** | 120 liters |
| **Weight, kg (min)** | 10 kg |
| **Payload** | 96 kg |
| **Material** | High density polyethylene HDPE, free of heavy metals, UV resistant |
| **Color** | Blue |
| **Body** | - Square section  Flaps-flat, adapted to the body,  Mounted in 2 points to the body with 2 screw pins, - 2 handles  - 2 rubber wheels of 200 mm diameter, anti-corrosive, static load treated over 100 kg, 1 (one) galvanized solid metal axe  - Frontal grip  - Resistance handle, designed on the lid for a comfortable grip  - Hinges assured |
| **Dimensions, mm (±5%)** | Width max. – 580  Length max. – 730  Height max. - 1100 |
| **Special construction element** | * 6 mm ribs extra enforcement on the upper part of the waste bin * wheels with solid rubber * strong bottom |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **LOT #3** | | | | | | |
| **Currency of the Quotation: MDL Moldovan Lei**  **INCOTERMS: DAP** | | | | | | |
| **Item No** | **Description** | | **UOM** | **Qty** | **Unit price** | **Total price** |
| **1** | **Waste plastic bin 1100 liters**  Mobile blue plastic containers for waste with 4 wheels, with blue flat lid with hole for paper introduction | | **unit** | **100** |  |  |
| **2** | **Waste plastic bin 1100 liters**  Mobile blue plastic container for waste with 4 wheels, with yellow flat lid with hole for plastic bottles introduction (size Ø 160 mm) | | **unit** | **75** |  |  |
|  | **Destination** | - waste collection and recycling  - waste bin with 4 wheels adapted for standard handling and lifting device, stable to ultraviolet radiation, rectangular section, flat hinge cover |  | | | |
|  | **Product certification** | Tested according to EN 840 – 1:2013, EN 840 – 5:2013, EN 840 – 6:2013 |
|  | **System certification** | Produced in integration quality management system according to ISO 9001, ISO 14001, Conformité Européene (CE) |
|  | **Volume, nominal** | 1100 liters |
|  | **Weight, kg (min)** | 50 kg |
|  | **Payload** | 440 kg |
|  | **Material** | High density polyethylene HDPE, free of heavy metals, UV resistant |
|  | **Color** | 100 units - blue bin with blue flat lid  75 units - blue bin with yellow flat lid |
|  | **Body** | - Square section  Flaps-flat, adapted to the body, Mounted in 2 points to the body with 2 screw pins, 2 handles  - Frontal grip  - Resistance handle, designed on the lid for a comfortable grip  - Hinges assured |
|  | **Dimensions, mm (±5%)** | Total height (max) – 1415;  Width (max) – 1380;  Length (max) – 1230;  Throw height (max) – 1165;  Wheel diameter – 200. |
|  | **Special construction element** | * 6 mm ribs extra enforcement on the upper part of the waste bin * 4 wheels (2 braked), non-marking solid rubber tires, directional locks for towing * reinforced wheel area   hand lever   * 100 units - blue bin with blue flat lid with hole for paper introduction * 75 units – blue bins with yellow flat lids with hole for introduction   plastic bottles (size Ø 160 mm) |

**Compliance with Requirements**

|  |  |  |  |
| --- | --- | --- | --- |
|  | **You Responses** | | |
| **Yes, we will comply** | **No, we cannot comply** | **If you cannot comply, pls. indicate counter - offer** |
| Maximum delivery period not to exceed 60 calendar days from the Contract signature |  |  | Click or tap here to enter text. |
| Minimum Technical Specifications |  |  | Click or tap here to enter text. |
| Delivery Term (INCOTERMS) |  |  | Click or tap here to enter text. |
| Validity of Quotation 90 calendar days |  |  | Click or tap here to enter text. |
| Minimum 12 months of warranty |  |  | Click or tap here to enter text. |
| Availability of certificates of quality, conformity and origin for the offered equipment |  |  | Click or tap here to enter text. |
| Payment terms |  |  | Click or tap here to enter text. |
| All Provisions of the UNDP General Terms and Conditions |  |  | Click or tap here to enter text. |

|  |  |
| --- | --- |
| I, the undersigned, certify that I am duly authorized to sign this quotation and bind the company below in event that the quotation is accepted. | |
| *Exact name and address of company*  Company NameClick or tap here to enter text.  Address: Click or tap here to enter text.  Click or tap here to enter text.  Phone No.: Click or tap here to enter text.  Email Address: Click or tap here to enter text. | Authorized Signature:  Date: Click or tap here to enter text.  Name: Click or tap here to enter text.  Functional Title of Authorised  Signatory: Click or tap here to enter text.  Email Address: Click or tap here to enter text. |