## **ANNEX 3: TECHNICAL AND FINANCIAL OFFER - GOODS**

*Bidders are requested to complete this form, sign it and return it as part of their bid along with Annex 2: Quotation Submission Form. The Bidder shall fill in this form in accordance with the instructions indicated. No alterations to its format shall be permitted and no substitutions shall be accepted.*

|  |  |
| --- | --- |
| Name of Bidder: | Click or tap here to enter text. |
| RFQ reference: | **RfQ21/02304: EU4MD/ Supply of Plastic waste bins – 120 liters (Lot #1), 240 liters (Lot #2) and 1100 liters (Lot #3)** | Date: Click or tap to enter a date. |

|  |
| --- |
| **LOT #1** |
| **Currency of the Quotation: USD** **INCOTERMS: DAP** |
| **Item No** | **Description** | **UOM** | **Qty** | **Unit price** | **Total price**  |
| **1** | **Waste plastic bin 120 liters**Mobile plastic containers for waste with 2 wheels, lifting appliances with fork | **unit** | **200** |  |  |
| **Destination** | - waste collection and recycling- waste bin with 2 wheels adapted for standard handling and lifting device, stable to ultraviolet radiation, rectangular section, flat hinge cover |
| **Product certification** | Tested according to EN 840 – 1:2013, EN 840 – 5:2013, EN 840 – 6:2013 |
| **System certification** | Produced in integration quality management system according to ISO 9001, ISO 14001 |
| **Volume, nominal** | 120 liters |
|  **Weight, kg (min)** | 7 kg |
| **Material** | High density polyethylene HDPE, free of heavy metals, UV resistant |
| **Color**  | Blue |
| **Body** | Square sectionFlaps-flat, adapted to the body,Mounted in 2 points to the body with 2 screw pins, 2 handles2 rubber wheels of 200 mm diameter, anti-corrosive, static load treated over 100 kg, 1 (one) galvanized solid metal axeFrontal gripResistance handle, designed on the lid for a comfortable gripHinges assured |
| **Dimensions, mm (±5%)** | Width max. – 480Length max. – 550Height max. - 1000 |
| **Special construction element** | 6 mm ribs extra enforcement on the upper part of the waste binwheels with solid rubberstrong bottom |

|  |
| --- |
| **LOT #2** |
| **Currency of the Quotation: USD****INCOTERMS: DAP** |
| **Item No** | **Description** | **UOM** | **Qty** | **Unit price** | **Total price**  |
| **1** | **Waste plastic bin 240 liters**Mobile plastic containers for waste with 2 wheels, lifting appliances with fork | **unit** | **100** |  |  |
| **Destination** | - waste collection and recycling- waste bin with 2 wheels adapted for standard handling and lifting device, stable to ultraviolet radiation, rectangular section, flat hinge cover |
| **Product certification** | Tested according to EN 840 – 1:2013, EN 840 – 5:2013, EN 840 – 6:2013 |
| **System certification** | Produced in integration quality management system according to ISO 9001, ISO 14001 |
| **Volume, nominal** | 240 liters |
|  **Weight, kg (min)** | 10 kg |
| **Payload** | 96 kg |
| **Material** | High density polyethylene HDPE, free of heavy metals, UV resistant |
| **Color**  | Blue |
| **Body** | - Square sectionFlaps-flat, adapted to the body,Mounted in 2 points to the body with 2 screw pins, - 2 handles- 2 rubber wheels of 200 mm diameter, anti-corrosive, static load treated over 100 kg, 1 (one) galvanized solid metal axe- Frontal grip- Resistance handle, designed on the lid for a comfortable grip- Hinges assured |
| **Dimensions, mm (±5%)** | Width max. – 580Length max. – 730Height max. - 1100 |
| **Special construction element** | * 6 mm ribs extra enforcement on the upper part of the waste bin
* wheels with solid rubber
* strong bottom
 |

|  |
| --- |
| **LOT #3** |
| **Currency of the Quotation: USD****INCOTERMS: DAP** |
| **Item No** | **Description** | **UOM** | **Qty** | **Unit price** | **Total price**  |
| **1** | **Waste plastic bin 1100 liters**Mobile blue plastic containers for waste with 4 wheels, with blue flat lid with hole for paper introduction | **unit** | **100** |  |  |
| **2** | **Waste plastic bin 1100 liters**Mobile blue plastic container for waste with 4 wheels, with yellow flat lid with hole for plastic bottles introduction (size Ø 160 mm)  | **unit** | **75** |  |  |
|  | **Destination** | - waste collection and recycling- waste bin with 4 wheels adapted for standard handling and lifting device, stable to ultraviolet radiation, rectangular section, flat hinge cover |  |
|  | **Product certification** | Tested according to EN 840 – 1:2013, EN 840 – 5:2013, EN 840 – 6:2013 |
|  | **System certification** | Produced in integration quality management system according to ISO 9001, ISO 14001, Conformité Européene (CE) |
|  | **Volume, nominal** | 1100 liters |
|  |  **Weight, kg (min)** | 50 kg |
|  | **Payload** | 440 kg |
|  | **Material** | High density polyethylene HDPE, free of heavy metals, UV resistant |
|  | **Color**  | 100 units - blue bin with blue flat lid 75 units - blue bin with yellow flat lid |
|  | **Body** | - Square sectionFlaps-flat, adapted to the body, Mounted in 2 points to the body with 2 screw pins, 2 handles- Frontal grip- Resistance handle, designed on the lid for a comfortable grip- Hinges assured |
|  | **Dimensions, mm (±5%)** | Total height (max) – 1415; Width (max) – 1380; Length (max) – 1230; Throw height (max) – 1165; Wheel diameter – 200. |
|  | **Special construction element** | * 6 mm ribs extra enforcement on the upper part of the waste bin
* 4 wheels (2 braked), non-marking solid rubber tires, directional locks for towing
* reinforced wheel area

hand lever* 100 units - blue bin with blue flat lid with hole for paper introduction
* 75 units – blue bins with yellow flat lids with hole for introduction

plastic bottles (size Ø 160 mm)  |

**Compliance with Requirements**

|  |  |
| --- | --- |
|  | **You Responses** |
|  | **Yes, we will comply** | **No, we cannot comply** | **If you cannot comply, pls. indicate counter - offer** |
| Maximum delivery period not to exceed 60 calendar days from the Contract signature  |[ ] [ ]  Click or tap here to enter text. |
| Minimum Technical Specifications |[ ] [ ]  Click or tap here to enter text. |
| Delivery Term (INCOTERMS) |[ ] [ ]  Click or tap here to enter text. |
| Validity of Quotation 90 calendar days |[ ] [ ]  Click or tap here to enter text. |
| Minimum 12 months of warranty |[ ] [ ]  Click or tap here to enter text. |
| Availability of certificates of quality, conformity and origin for the offered equipment |[ ] [ ]  Click or tap here to enter text. |
| Payment terms |[ ] [ ]  Click or tap here to enter text. |
| All Provisions of the UNDP General Terms and Conditions |[ ] [ ]  Click or tap here to enter text. |

|  |
| --- |
| I, the undersigned, certify that I am duly authorized to sign this quotation and bind the company below in event that the quotation is accepted. |
| *Exact name and address of company*Company NameClick or tap here to enter text.Address: Click or tap here to enter text. Click or tap here to enter text.Phone No.: Click or tap here to enter text.Email Address: Click or tap here to enter text. | Authorized Signature: Date: Click or tap here to enter text.Name: Click or tap here to enter text.Functional Title of Authorised Signatory: Click or tap here to enter text.Email Address: Click or tap here to enter text. |