**ANNEX 4. Technical Responsiveness Table for Camera Surveillance Systems**

**Bidders shall provide all the applicable data of the equipment offered, failing to do so may result in the bid being rejected. Corresponding documentation shall form part of the bidder’s offer.**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Item Description** | **Specifications** | **√**  **Yes** | **√**  **No** | **Technical Compliance**  **Please provide details /description of offered feature)** |
| 1 | **Indoor Camera** | - Minimum of 4 Mega Pixel Analog Camera  - Minimum Frame Rate of 2688×1520 at 20fps  - Minimum Illumination of Color mode 0.8 Lux and 0 Lux with IR mode  - Lens size 2.8mm or 3.6mm  - viewing/wide angle: min 80 °  - IR range: minimum 30 meters  - Support WDR  - Operating Humidity from 10% to 90%  - Day & Night: IR cut filter  - Synchronization: Internal synchronization  - AGC: Support  - D/N Mode: Auto/Color/BW (Black and White)  - White Balance: ATW/MWB  - BLC: Support  - Functions: Brightness, Sharpness, DNR, Mirror, Smart IR  - Power Supply: 12 VDC ±25%, PoE  - Power Consumption: Max. 5 W  - Material: Plastic  - Accessories: Mountable Bracket allowing both ceiling and wall options |  |  |  |
| 2 | **Digital Video Recorder** | - 4-channels analog video input  - 4 Mega Pixel video input resolution  - 4 Mega Pixel Video recording and Playback  - Support H.265+/H.265/H.264 ++/H.264 Video Compression  - Support frame rate of 25fps at 4 Mega Pixel mainstream  - Support Network Protocols TCP/IP, DHCP, DNS, DDNS, NTP, NFS, iSCSI, UPnP, HTTPS, ONVIF  - Support SATA interfaces of a Minimum 1 Slot  - Support Hard Disk Size of minimum 3 TB size at each slot  - Support Network interface minimum of 1 port RJ45 10M/100M self-adaptive Ethernet interface  - Has a minimum of 2 USB Ports, one of them shall be at front side  - Working temperature from -10 ºC to +55 ºC  - Working Humidity from 10% to 90%  - HDMI output interface with a minimum 1920 × 1080/60Hz resolution  - VGA output interface with a minimum 1920 × 1080/60Hz resolution |  |  |  |
| 3 | **Hard Disk Drive** | - Internal SATA 3.5 inches Hard Drive  - Size of minimum 3 Terabytes for 24/7 Surveillance mode  - 5400 RPM Performance Class  - 6 Gb/s SATA interface buffer  - Cash Size 64 MB |  |  |  |
| 4 | **POE Switch** | - 4 POE ports 10/100 Mbps  - 1 uplink port  - Individual LED indicator for each output  - Min POE port power Consumption: Max. 30 W  - Power Supply |  |  |  |
| 5 | **Full Installation that includes:** | - Supply, install, connect and commission surveillance and recording System, including all required works, decorative trunk, conduits, cables, wires and fittings, steel poles for external CAM, related civil works |  |  |  |
| 6 | **Training** | - Training for 2 Administrators (1 from each region) is needed.  - Training length shall not be less than 1 hour |  |  |  |
| 7 | **Warranty period** | Warranty for a minimum period of 24 months on both parts and labor |  |  |  |

|  |  |
| --- | --- |
| I, the undersigned, certify that I am duly authorized to sign this quotation and bind the company below in event that the quotation is accepted. | |
| *Exact name and address of company*  Company NameClick or tap here to enter text.  Address: Click or tap here to enter text.  Click or tap here to enter text.  Phone No.: Click or tap here to enter text.  Email Address: Click or tap here to enter text. | Authorized Signature:  Date: Click or tap here to enter text.  Name: Click or tap here to enter text.  Functional Title of Authorised  Signatory: Click or tap here to enter text.  Email Address: Click or tap here to enter text. |