**Annex 2**

**FORM FOR SUBMITTING SUPPLIER’S QUOTATION**

***(This Form must be submitted only using the Supplier’s Official Letterhead/Stationery)***

We, the undersigned, hereby accept in full the UNDP General Terms and Conditions, and hereby offer to supply the items listed below in conformity with the specification and requirements of UNDP as per RFQ Reference No. 17/01507:

**TABLE 1: Offer to Supply Goods Compliant with Technical Specifications and Requirements**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item No.** | **Description/Specification of Goods** | **Q-ty** | **Unit Price, USD** | **Total Price per Item, USD** |
| **A.** | **Motorola TETRA Portable Radios and Accessories (Warranty – 2 years for terminals; 1 year – for accessories)** | | | |
| 1 | MTP3500 TETRA Portable Radio:   * High capacity battery (2150mAh); * Frequency band: at least 380-400 MHz; * TEA1; * Dust and water ingress protection – IP67; * User manual in Romanian and/or English. | 32 pcs |  |  |
| 2 | MTP3550 TETRA Portable Radio:   * High capacity battery (2150mAh); * Frequency band: at least 380-400 MHz; * TEA1; * Dust and water ingress protection – IP67; * User manual in Romanian and/or English. | 10 pcs |  |  |
| 3 | 2’’ Belt clip (PMLN5616) | 42 pcs |  |  |
| 4 | Antenna Stubby 380-430 MHz 55mm (85012056001) | 42 pcs |  |  |
| 5 | 2150 mAh high-capacity Li-Ion battery, IP55 (NNTN8023) | 42 pcs |  |  |
| 6 | Personal radio charger with Euro Plug (PS000042A32) | 5 pcs |  |  |
| 7 | Desktop dual-unit charger for charging radio and spare battery simultaneously (Euro plug) (PMLN6494) | 10 pcs |  |  |
| 8 | Multi-unit charger with 6 battery pockets (Euro plug) (NNTN8152) | 6 pcs |  |  |
| 9 | Battery charging insert for multi-unit battery charger (NNTN8037) | 36 pcs |  |  |
| 10 | Bluetooth accessories: |  |  |  |
|  | - single-wire surveillance kit (PMLN7052) | 42 pcs |  |  |
|  | - wireless push-to-talk (PTT) pod (NNTN8191) | 42 pcs |  |  |
|  | - mini USB charging plug with Euro plug (PMPN4006) | 42 pcs |  |  |
| 11 | Licenses, Security Options: | 42 pcs (or a solution for 42 terminals) |  |  |
|  | - Bluetooth (if not included by default in MTP3500/3550 TETRA Portable Radio) |  |  |  |
|  | - GPS (if not included by default in MTP3500/3550 TETRA Portable Radio) |  |  |  |
|  | - Man Down functionality (if not included by default in MTP3500/3550 TETRA Portable Radio) |  |  |  |
|  | - End-to-End Encryption (if not included by default in MTP3500/3550 TETRA Portable Radio) |  |  |  |
| 12 | Configuration/programming kit: cable and software | 3 pcs |  |  |
| 13 | Support in configuration of terminals; Training of end user |  |  |  |
| **B.** | **Motorola TETRA Mobile Radios and Accessories (Warranty – 2 years for terminals; 1 year – for accessories)** | | | |
| 1 | MTM5400 TETRA Mobile Radio Station:   * Dash mount; * Frequency band: at least 380-400 MHz; * TEA1; * Gateway Repeater Functionality; * User manual in Romanian and/or English. | 4 pcs |  |  |
| 2 | TETRA/GPS Antenna 380-400 MHz (mounts and cables included) | 4 pcs |  |  |
| 3 | Heavy Duty Microphone (RMN5111) | 4 pcs |  |  |
| 4 | External Speaker (RSN4002A) | 4 pcs |  |  |
| 5 | Power supply and other connection cables | 4 pcs |  |  |
| 6 | Configuration/programming kit: cable and software | 2 pcs |  |  |
| 7 | Licenses, Security Options: | 4 pcs (or a solution for 4 terminals) |  |  |
|  | - GPS (if not included by default in MTM5400TETRA Mobile Radio) |  |  |  |
|  | - End-to-End Encryption (if not included by default in MTM5400TETRA Mobile Radio) |  |  |  |
| 8 | Support in configuration of terminals; Training of end user |  |  |  |
|  | **Total Prices of Goods** | | |  |
|  | Add: Cost of Transportation | | |  |
|  | Add: Cost of Installation | | |  |
|  | Add: Other Charges (pls. specify) | | |  |
|  | **Total Final and All-Inclusive Price Quotation** | | |  |

**TABLE 2: Offer to Comply with Other Conditions and Related Requirements**

|  |  |  |  |
| --- | --- | --- | --- |
| **Other Information pertaining to our Quotation are as follows:** | **Your Responses** | | |
| ***Yes, we will comply*** | ***No, we cannot comply*** | ***If you cannot comply, pls. indicate counter proposal*** |
| Delivery Lead Time: up to 90 calendar days upon signature of contract |  |  |  |
| Warranty and After-Sales Requirements |  |  |  |
| 1. Minimum 2 (two) years for TETRA terminals and 1 (one) year for accessories 2. Brand new replacement if Purchased Unit is beyond repair |  |  |  |
| Validity of Quotation: 90 calendar days |  |  |  |
| All Provisions of the UNDP General Terms and Conditions |  |  |  |

All other information that we have not provided automatically implies our full compliance with the requirements, terms and conditions of the RFQ.

*[Name and Signature of the Supplier’s Authorized Person]*

*[Designation]*

*[Date]*