**ANNEX 2**

# QUOTATION SUBMISSION FORMS

**STATEMENT OF CONFIRMATION**

***[The supplier shall fill in this form with no alterations or substitutions to its format and content]***

To: *UN Women,*

*131, 31 August 1989,* Date: *[insert date of Quotation Submission]*

*Chisinau, Moldova*

We, the undersigned, declare that:

1. We (representatives of this company, inclusive of any associated legal representatives) have examined the minimum requirements, terms and clauses and have no reservations to the RFQ including all annexes*;*
2. We agree to abide by this RFQ and in accordance with the UN Women General Conditions of Contract (Annex IV) and will not request any changes to the existing terms, conditions and clauses;
3. We offer to supply in conformity with the **RFQ17/01588**, the following **supply and installation of glass partitions and glass doors for UN Women Moldova**, and undertake, if our offer is accepted, to commence and complete delivery of all goods specified in the contract within the time frame stipulated;
4. We offer to supply for the sum as may be ascertained in accordance with the Quotation submitted and with the instructions under the Quotation Instruction Sheet;
5. Our offer shall be valid for a period of **60 days** from the date fixed for opening the RFQ, and it shall remain binding upon us and may be accepted at any time before the expiration of that period;
6. We understand that UN Women is not bound to accept the lowest evaluated quotation or any other quotation that you may receive.

|  |  |
| --- | --- |
| **SIGNATURE AND CONFIRMATION OF THE RFQ** | |
| PROVIDED THAT A PURCHASE ORDER IS ISSUED BY UN WOMEN **WITHIN THE QUOTATION VALIDITY PERIOD** **STATED ABOVE**, THE UNDERSIGNED HEREBY COMMITS, SUBJECT TO THE TERMS OF SUCH PURCHASE ORDER, TO FURNISH ANY OR ALL ITEMS AT THE PRICES OFFERED AND TO DELIVER SAME TO THE DESIGNATED POINT(S) WITHIN THE DELIVERY TIME STATED ABOVE. THE UNDERSIGNED HEREBY SIGNS IN CONFIRMATION THAT THEY HAVE REVIEWED THE RFQ AND AGREE TO UN WOMEN CONTRACT MODEL AND THE GENERAL CONDITIONS OF CONTRACT. | |
| *Exact name and address of company*  COMPANY NAME:  ADDRESS:    PHONE NO.: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  E-MAIL ADDRESS: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | AUTHORIZED SIGNATURE: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  DATE: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  NAME: (TYPE OR PRINT) \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  FUNCTIONAL TITLE OF AUTHORIZED SIGNATORY: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  E-MAIL ADDRESS: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| **This quotation submission form MUST be duly completed and returned with the QUOTATION, along with confirmation that the products are in accordance with specifications and requirements of UN Women. The quotation “MUST” be submitted in the vendor’s business letterhead stationery. Failure to do so may result in disqualification of your QUOTATION.** | |

**Quotation Format**

**TABLE 1: Offer to provide Supply and Installation of Glass Partitions and Glass Doors for**

**UN Women Moldova Compliant with Technical Specifications and Requirements**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **UNIT PRICES (Indicate the Price & Currency of Quotation):** | | | | | |
| ITEM | DESCRIPTION | QTY. | UNIT OF MEASURE | CURRENCY, **MDL:** | |
| UNIT PRICE,  (including shipping installation) | TOTAL PRICE,  (including shipping installation) |
| 1. | Установка стеклянной перегородки в лифтовом холле. Пол в помещении- плитка керамическая, потолок-ARMSTRONG.  Длина перегородки (с дверью) 3,25 м, высота перегородки 2415 мм, размер двухстворчатой двери 1400х2100мм. Полотна двери открываются в обе стороны, оборудованы доводчиками и стопорами, позволяющими двери оставаться при полном открывании в открытом положении. Дверь не закрывается на ключ.  Перегородка выполняется из закаленного безопасного стекла. Толщина стекла 10 мм для двери и для перегородки. Примерная ширина отдельных секций 900- 1000 мм. Зазоры между секциями и угловые примыкания выполняются через прозрачные пластиковые элементы. Стеклянная перегородка и дверь полностью прозрачные, вехняя и нижняя направляющая высотой около 40 мм. | 1 | шт |  |  |
| 2. | Замена существующей стеклянной двери в основное офисное пространство на новую дверь (с установкой).  Проем 1380х2156. Дверь полностью матовая (пленка ОRACAL). Полотна двери открываются в обе стороны, оборудованы доводчиками и стопорами, позволяющими двери оставаться при полном открывании в открытом положении. Дверь закрывается на ключ. Рассмотреть возможность закрывания двери на электронный замок. | 1 | шт |  |  |
| 3. | Установка стеклянных перегородок в основном пространстве офиса. Пол в помещении- линолеум ПВХ, потолок-ARMSTRONG.  Общая длина стеклянных перегородок с дверными проемами 48,5 м п. Перегородки выполняются из закаленного безопасного стекла. Толщина стекла 10 мм для дверей и для перегородок. Примерная ширина отдельных секций 900- 1000 мм. Зазоры между секциями и угловые соединения выполняются через прозрачные пластиковые элементы. Верхняя и нижняя направляющая высотой около 40 мм. Общее количество дверей размером 900х 2100 в стеклянных перегородках 8 штук. Двери оборудованы доводчиками и стопорами, позволяющими двери оставаться при полном открывании в открытом положении.  На стеклянные перегородки и двери наклеиваются горизонтальные полосы из матовой пленки ОRACAL. Высота полос 1000мм,150мм,150мм. Полосы наклеиваются с интервалом 100 мм. | 48,5 | метр погонный |  |  |
| 4. | Установка стеклянных дверей в проемы 900 х2100 в гипсокартоновых перегородках. Общее количество дверей 2 штуки. Двери полностью матовые (пленка ОRACAL). Полотно открывается в обе стороны, двери оборудованы доводчиками и стопорами, позволяющими полотну двери оставаться при полном открывании в открытом положении. | 2 | шт |  |  |

|  |  |
| --- | --- |
| **TOTAL PRICES (Indicate the Price & Currency of Quotation)** | |
| TOTAL DAPPRICE: |  |
| FREIGHT /INSURANCE/HANDLING COSTS: |  |
| TOTAL COST: |  |

**TABLE 2: Compliance Requirements**

|  |  |  |  |
| --- | --- | --- | --- |
| **Compliance Requirements :** | **Your Responses** | | |
| ***Yes, we will comply*** | ***No, we cannot comply*** | ***Provide reasons for non-compliance*** |
| Payment terms: as per provisions of Request for Quotations |  |  |  |
| Delivery Lead Time: *30 calendar days upon signature of contract* |  |  |  |
| Validity Period of Quotation: 6*0 days* |  |  |  |
| Warranty and After-Sales Requirements |  |  |  |
| 1. Instructions on operations and maintenance |  |  |  |
| 1. Minimum two (2) year warranty on both parts and labor |  |  |  |
| All Provisions of the UN Women General Terms and Conditions |  |  |  |

All other information that we have not provided automatically implies our full compliance with the requirements, terms and conditions of the RFQ.