**Annex 2**

**FORM FOR SUBMITTING SUPPLIER’S QUOTATION**

***(This Form must be submitted only using the Supplier’s Official Letterhead/Stationery[[1]](#footnote-1))***

We, the undersigned, hereby accept in full the UNDP General Terms and Conditions, and hereby offer to supply the items listed below in conformity with the specification and requirements of UNDP as per RFQ Reference No. **RfQ-18/01736 – Supply of 1 (one) Waste Disposal Truck with back loading**.

|  |
| --- |
| **LOT #1** |

**TABLE 1: Offer to Supply Equipment Compliant with Technical Specifications and Requirements**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Item No.** | **Description/Specification of equipment** | **Quantity** | **Latest Delivery Date** | **Unit Price** | **Total Price per Item** |
|  | **Waste truck** | 1 | 90 days |  |  |
|  | **Total Price[[2]](#footnote-2)** | | | |  |
|  | Add: Cost of Transportation | | | |  |
|  | Add: Cost of Insurance | | | |  |
|  | Add: Other Charges (pls. specify) | | | |  |
|  | **Total Final and All-Inclusive Price Quotation (USD, VAT 0%)** | | | |  |

**TABLE 2: Estimated Operating Costs (consumables and spares, including their prices and details on local availability for the first 1,000 motor-hours) \***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **List of Consumable Item/s**  **(if applicable)** | **Motor-hours when servicing is required** | **List of replacement parts required** | **Cost of replacement parts** | **Cost of maintenance works** | **Total Price per Item**  **(USD, VAT 0%)** |
| Motor Oil |  |  |  |  |  |
| Oil filter |  |  |  |  |  |
| Gearbox Oil |  |  |  |  |  |
| Timing Belt |  |  |  |  |  |
| Generator belt |  |  |  |  |  |
| Belt tensioner and pulleys |  |  |  |  |  |
| Spark Plugs |  |  |  |  |  |
| Air filter |  |  |  |  |  |
| Salon filter |  |  |  |  |  |
| Brake pads |  |  |  |  |  |
| **Total Cost** | | | | | **USD** |

\**These costs shall be quoted based on current prices at a local authorized service centre and shall be taken into account by UNDP during the evaluation process to calculate the life cycle cost of the vehicle. These maintenance services shall not be contracted by UNDP at this stage. The contract shall contain only the vehicles, warranty, delivery and other related charges.*

**TABLE 3 : Offer to Comply with Other Conditions and Related Requirements**

|  |  |  |  |
| --- | --- | --- | --- |
| **Other Information pertaining to our Quotation are as follows:** | **Your Responses** | | |
| ***Yes, we will comply*** | ***No, we cannot comply*** | ***If you cannot comply, pls. indicate counter proposal*** |
| Delivery Lead Time (up to 90 calendar days from PO contract signature) |  |  |  |
| Warranty and After-Sales Requirements |  |  |  |
| 1. Minimum 24 months or 100,000 km on both parts and labor |  |  |  |
| 1. Availability of certificates of quality and origin for the offered equipment |  |  |  |
| 1. Availability of authorized service in Moldova |  |  |  |
| Validity of Quotation: 60 calendar days |  |  |  |
| All Provisions of the UNDP General Terms and Conditions |  |  |  |

**TABLE 4 : Technical Responsiveness Table**

Bidders shall provide all the applicable data of the equipment offered, failing to do so may result in the bid being rejected. Corresponding documentation shall form part of the bidder’s offer.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | Item Description | Specifications | √  Yes | √  No | Technical Compliance  Please provide details /description of offered feature) |
| 1 | Waste Disposal Truck | |  |  |  |
| Condition | Brand New, year of production 2018 |  |  |  |
| Dimensions | Length, mm: max. 7500  Width, mm: max. 2600  Height, mm: max. 3500 |  |  |  |
| Total vehicle weight, kg | max. 13500 |  |  |  |
| Fuel | Diesel |  |  |  |
| Engine Horsepower, HP | min. 149 |  |  |  |
| European emission standards | Min. “Euro 3” |  |  |  |
| Steering | Steering mechanism with the hydraulic booster |  |  |  |
| Standard equipment | Spare wheel. First aid kit. Emergency triangle and lantern, lifting jack. The bracket for the installation of fire extinguishers. Set of tools. |  |  |  |
| Warranty | 24 months |  |  |  |
| Technical specifications of the waste container | |  |  |  |
| Loading type | Back loading |  |  |  |
| Capacity of load container, m3 | Min. 9 |  |  |  |
| Mass of loaded waste, kg | min. 3600 |  |  |  |
| Types of loadable dustbins, liters (euro-standards) | Small dustbins – minimum 120 litters;  Big dustbins - minimum 750 litters; |  |  |  |
| Additional options | Footboards and handles for operators |  |  |  |

All other information that we have not provided automatically implies our full compliance with the requirements, terms and conditions of the RFQ.

*[Name and Signature of the Supplier’s Authorized Person]*

*[Designation] \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ [Date]*

1. *Official Letterhead/Stationery must indicate contact details – addresses, email, phone and fax numbers – for verification purposes*  [↑](#footnote-ref-1)
2. *Pricing of goods should be consistent with the INCO Terms indicated in the RFQ* [↑](#footnote-ref-2)